<?xml version="1.0" encoding="UTF-8" standalone="no"?>
<SensorML xmlns="http://www.opengis.net/sensorML/1.0.1" xmlns:gml="http://www.opengis.net/gml" xmlns:swe="http://www.opengis.net/swe/1.0.1" xmlns:xlink="http://www.w3.org/1999/xlink" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" version="1.0.1" xsi:schemaLocation="http://www.opengis.net/sensorML/1.0.1 http://schemas.opengis.net/sensorML/1.0.1/sensorML.xsd">
	<member>
		<System>
			<gml:description>Weather station located on the roof of the
				Insititute for Geoinformatics of the University Münster, Germany.</gml:description>
			<keywords>
				<KeywordList>
					<keyword>weather station</keyword>
					<keyword>precipitation</keyword>
					<keyword>wind speed</keyword>
					<keyword>temperature</keyword>
					<keyword>barometric pressure</keyword>
					<keyword>luminance</keyword>
					<keyword>relative humidity</keyword>
					<keyword>Münster</keyword>
				</KeywordList>
			</keywords>
			<!--~~~~~~~~~~~~~~-->
			<!--Identification-->
			<!--~~~~~~~~~~~~~~-->
			<identification>
				<IdentifierList>
					<identifier name="uniqueID">
						<Term definition="urn:ogc:def:identifier:OGC:1.0:uniqueID">
							<value>urn:ogc:object:feature:OSIRIS-HWS:3d3b239f-7696-4864-9d07-15447eae2b93</value>
						</Term>
					</identifier>
					<identifier name="longName">
						<Term definition="urn:ogc:def:identifier:OGC:1.0:longName">
							<value>This is a WS2500 weather station setup at the Institute
								for Geoinformatics of the University of Münster</value>
						</Term>
					</identifier>
					<identifier name="shortName">
						<Term definition="urn:ogc:def:identifier:OGC:1.0:shortName">
							<value>IFGI HWS 1</value>
						</Term>
					</identifier>
					<identifier name="productName">
						<Term definition="urn:ogc:def:identifier:OGC:1.0:productName">
							<value>ELV Radio Weather Station WS 2500</value>
						</Term>
					</identifier>
					<identifier name="modelNumber">
						<Term definition="urn:ogc:def:identifier:OGC:1.0:modelNumber">
							<value>53759</value>
						</Term>
					</identifier>
					<identifier name="manufacturer">
						<Term definition="urn:ogc:def:identifier:OGC:1.0:manufacturer">
							<value>ELV Elektronik AG</value>
						</Term>
					</identifier>
					<identifier name="operator">
						<Term definition="urn:ogc:def:identifier:OGC:1.0:operator">
							<value>Institute for Geoinformatics, Muenster, Germany.</value>
						</Term>
					</identifier>
				</IdentifierList>
			</identification>
			<!--~~~~~~~~~~~~~~-->
			<!--Classification-->
			<!--~~~~~~~~~~~~~~-->
			<classification>
				<ClassifierList>
					<classifier name="intendedApplication">
						<Term definition="urn:ogc:def:classifier:OGC:1.0:application">
							<value>weather</value>
						</Term>
					</classifier>
					<classifier name="sensorType">
						<Term definition="urn:ogc:def:classifier:OGC:1.0:sensorType">
							<value>thermometer</value>
						</Term>
					</classifier>
					<classifier name="sensorType">
						<Term definition="urn:ogc:def:classifier:OGC:1.0:sensorType">
							<value>rain gauge</value>
						</Term>
					</classifier>
					<classifier name="sensorType">
						<Term definition="urn:ogc:def:classifier:OGC:1.0:sensorType">
							<value>barometer</value>
						</Term>
					</classifier>
					<classifier name="sensorType">
						<Term definition="urn:ogc:def:classifier:OGC:1.0:sensorType">
							<value>anemometer</value>
						</Term>
					</classifier>
					<classifier name="sensorType">
						<Term definition="urn:ogc:def:classifier:OGC:1.0:sensorType">
							<value>Luminance Sensor</value>
						</Term>
					</classifier>
				</ClassifierList>
			</classification>
			<!--~~~~~~~~~~-->
			<!--Valid time-->
			<!--~~~~~~~~~~-->
			<validTime>
				<gml:TimePeriod>
					<gml:beginPosition>2010-01-01</gml:beginPosition>
					<gml:endPosition>2011-12-31</gml:endPosition>
				</gml:TimePeriod>
			</validTime>
			<!--~~~~~~~~~~~~-->
			<!--Capabilities-->
			<!--~~~~~~~~~~~~-->
			<capabilities>
				<swe:DataRecord definition="urn:ogc:def:property:capabilities">
					<!--station is collecting data-->
					<swe:field name="status">
						<swe:Boolean definition="urn:ogc:def:property:OGC:1.0:isActive">
							<swe:value>true</swe:value>
						</swe:Boolean>
					</swe:field>
					<swe:field name="mobile">
						<swe:Boolean definition="urn:ogc:def:property:OGC:1.0:isMobile">
							<swe:value>false</swe:value>
						</swe:Boolean>
					</swe:field>
					<swe:field name="measuringInterval">
						<swe:Quantity definition="urn:ogc:def:property:OGC:1.0:measuringInterval">
							<gml:description>The measuring interval of the weather station.</gml:description>
							<swe:uom code="min" xlink:href="urn:ogc:def:uom:UCUM::min"/>
							<swe:value>3</swe:value>
						</swe:Quantity>
					</swe:field>
					<swe:field name="transmissionFrequency">
						<swe:Quantity definition="urn:ogc:def:property:OGC:1.0:transmissionFrequency">
							<gml:description>The transmission frequency of the weather
								station.</gml:description>
							<swe:uom code="MHz" xlink:href="urn:ogc:def:uom:UCUM::MHz"/>
							<swe:value>433.92</swe:value>
						</swe:Quantity>
					</swe:field>
					<swe:field name="powerSupply">
						<swe:Text definition="urn:ogc:def:property:OGC:1.0:powerSupply">
							<gml:description>The power supply of the weather station.</gml:description>
							<swe:value>4 Baby cells 1.5V = 7,5 V / 500 mA</swe:value>
						</swe:Text>
					</swe:field>
					<swe:field name="observedBBOX">
						<swe:Envelope definition="urn:ogc:def:property:OGC:1.0:observedBBOX" referenceFrame="urn:ogc:def:crs:EPSG:4326">
							<swe:lowerCorner>
								<swe:Vector>
									<swe:coordinate name="latitude">
										<swe:Quantity axisID="y">
											<swe:uom code="deg" xlink:href="urn:ogc:def:uom:UCUM::deg"/>
											<swe:value>51.939795</swe:value>
										</swe:Quantity>
									</swe:coordinate>
									<swe:coordinate name="longitude">
										<swe:Quantity axisID="x">
											<swe:uom code="deg" xlink:href="urn:ogc:def:uom:UCUM::deg"/>
											<swe:value>7.608445</swe:value>
										</swe:Quantity>
									</swe:coordinate>
								</swe:Vector>
							</swe:lowerCorner>
							<swe:upperCorner>
								<swe:Vector>
									<swe:coordinate name="latitude">
										<swe:Quantity axisID="y">
											<swe:uom code="deg" xlink:href="urn:ogc:def:uom:UCUM::deg"/>
											<swe:value>51.941978</swe:value>
										</swe:Quantity>
									</swe:coordinate>
									<swe:coordinate name="longitude">
										<swe:Quantity axisID="x">
											<swe:uom code="deg" xlink:href="urn:ogc:def:uom:UCUM::deg"/>
											<swe:value>7.612007</swe:value>
										</swe:Quantity>
									</swe:coordinate>
								</swe:Vector>
							</swe:upperCorner>
						</swe:Envelope>
					</swe:field>
				</swe:DataRecord>
			</capabilities>
			<!--~~~~~~~-->
			<!--Contact-->
			<!--~~~~~~~-->
			<contact>
				<ResponsibleParty gml:id="IfGI_contact">
					<individualName>Jürrens, Eike Hinderk</individualName>
					<organizationName>Institute for Geoinformatics, Münster,
						Germany.</organizationName>
					<contactInfo>
						<phone>
							<voice>+49 251 83 30088</voice>
							<facsimile>+49 251 83 39763</facsimile>
						</phone>
						<address>
							<deliveryPoint>Weselerstraße 253</deliveryPoint>
							<city>Münster</city>
							<administrativeArea>North Rhine-Westfalia</administrativeArea>
							<postalCode>49151</postalCode>
							<country>Germany</country>
							<electronicMailAddress>ehjuerrens@uni-muenster.de</electronicMailAddress>
						</address>
					</contactInfo>
				</ResponsibleParty>
			</contact>
			<documentation xlink:role="urn:ogc:def:object:OGC:1.0:image">
				<Document>
					<gml:description>photo of the weather station</gml:description>
					<format>image/jpg</format>
					<onlineResource xlink:href="http://ifgi.uni-muenster.de/~e_juer01/WS2500.jpg"/>
				</Document>
			</documentation>
			<!--in later SOS version this will be editable via the T-interface-->
			<history>
				<EventList>
					<member name="deployDate">
						<Event>
							<date>2007-06-01</date>
							<gml:description>Event of deploying the weather station.</gml:description>
							<contact xlink:href="#IfGI_contact"/>
						</Event>
					</member>
				</EventList>
			</history>
			<!--~~~~~~~~~-->
			<!--Position -->
			<!--~~~~~~~~~-->
			<spatialReferenceFrame>
				<gml:EngineeringCRS gml:id="STATION_FRAME">
					<gml:srsName>Spatial Reference System of station</gml:srsName>
					<gml:usesCS xlink:href="urn:ogc:def:cs:OGC:1.0:Grid2dSquareCS"/>
					<gml:usesEngineeringDatum>
						<gml:EngineeringDatum gml:id="STATION_DATUM">
							<gml:datumName>Spatial Datum of station</gml:datumName>
							<gml:anchorPoint>Origin is the base of the station.
								Z is vertical.
								X and Y are orthogonal to Z.
								X is orthogonal to Y.
								Y is parallel to the North-Axis and points to North.
								X is orthogonal to the North-Axis and points to East.</gml:anchorPoint>
						</gml:EngineeringDatum>
					</gml:usesEngineeringDatum>
				</gml:EngineeringCRS>
			</spatialReferenceFrame>
			<position name="stationPosition">
				<swe:Position fixed="false" referenceFrame="urn:ogc:def:crs:EPSG:4326">
					<swe:location>
						<swe:Vector gml:id="STATION_LOCATION">
							<swe:coordinate name="latitude">
								<swe:Quantity axisID="y">
									<swe:uom code="deg" xlink:href="urn:ogc:def:uom:UCUM::deg"/>
									<swe:value>51.9412</swe:value>
								</swe:Quantity>
							</swe:coordinate>
							<swe:coordinate name="longitude">
								<swe:Quantity axisID="x">
									<swe:uom code="deg" xlink:href="urn:ogc:def:uom:UCUM::deg"/>
									<swe:value>7.6103</swe:value>
								</swe:Quantity>
							</swe:coordinate>
							<swe:coordinate name="altitude">
								<swe:Quantity axisID="z">
									<swe:uom code="m" xlink:href="urn:ogc:def:uom:UCUM::m"/>
									<swe:value>200</swe:value>
								</swe:Quantity>
							</swe:coordinate>
						</swe:Vector>
					</swe:location>
				</swe:Position>
			</position>
			<!--~~~~~~~~~~~~~~~~~-->
			<!--System Interfaces-->
			<!--~~~~~~~~~~~~~~~~~-->
			<interfaces>
				<InterfaceList>
					<interface name="IFGI-WeatherSOS">
						<InterfaceDefinition>
							<serviceLayer>
								<swe:DataRecord definition="urn:ogc:def:interface:OGC:1.0:SWEServiceInterface">
									<swe:field name="urn:ogc:def:interface:OGC:1.0:ServiceURL">
										<swe:Text>
											<swe:value>http://v-swe.uni-muenster.de:8080/WeatherSOS/sos
										</swe:value>
										</swe:Text>
									</swe:field>
									<swe:field name="urn:ogc:def:interface:OGC:1.0:ServiceType">
										<swe:Text>
											<swe:value>SOS</swe:value>
										</swe:Text>
									</swe:field>
									<swe:field name="urn:ogc:def:interface:OGC:1.0:ServiceSpecificSensorID">
										<swe:Text>
											<swe:value>urn:ogc:object:feature:OSIRIS-HWS:3d3b239f-7696-4864-9d07-15447eae2b93</swe:value>
										</swe:Text>
									</swe:field>
								</swe:DataRecord>
							</serviceLayer>
						</InterfaceDefinition>
					</interface>
				</InterfaceList>
			</interfaces>
			<!--~~~~~~~~~~~~~-->
			<!--System Inputs-->
			<!--~~~~~~~~~~~~~-->
			<inputs>
				<InputList>
					<input name="precipitation">
						<swe:ObservableProperty definition="urn:ogc:def:property:OGC::Precipitation"/>
					</input>
					<input name="atmosphericTemperature">
						<swe:ObservableProperty definition="urn:ogc:def:property:OGC::AirTemperature"/>
					</input>
					<input name="atmosphericPressure">
						<swe:ObservableProperty definition="urn:ogc:def:property:OGC::AtmosphericPressure"/>
					</input>
					<input name="wind">
						<swe:ObservableProperty definition="urn:ogc:def:property:OGC::Wind"/>
					</input>
					<input name="luminance">
						<swe:ObservableProperty definition="urn:ogc:def:property:OGC::Luminance"/>
					</input>
					<input name="humidity">
						<swe:ObservableProperty definition="urn:ogc:def:property:OGC::RelativeHumidity"/>
					</input>
				</InputList>
			</inputs>
			<!--~~~~~~~~~~~~~~-->
			<!--System Outputs-->
			<!--~~~~~~~~~~~~~~-->
			<outputs>
				<OutputList>
					<output name="precipitation">
						<swe:Quantity definition="urn:ogc:def:property:OGC::Precipitation1Hour">
							<gml:metaDataProperty>
								<offering>
									<id>RAIN_GAUGE</id>
									<name>Rain</name>
								</offering>
							</gml:metaDataProperty>
							<swe:uom code="mm" xlink:href="urn:ogc:def:uom:UCUM::mm"/>
						</swe:Quantity>
					</output>
					<output name="windDirection">
						<swe:Quantity definition="urn:ogc:def:property:OGC::WindDirection">
							<gml:metaDataProperty>
								<offering>
									<id>WIND_DIRECTION</id>
									<name>Direction of the wind</name>
								</offering>
							</gml:metaDataProperty>
							<swe:uom code="deg" xlink:href="urn:ogc:def:uom:UCUM::deg"/>
						</swe:Quantity>
					</output>
					<output name="windSpeed">
						<swe:Quantity definition="urn:ogc:def:property:OGC::WindSpeed">
							<gml:metaDataProperty>
								<offering>
									<id>WIND_SPEED</id>
									<name>Speed of the wind</name>
								</offering>
							</gml:metaDataProperty>
							<swe:uom code="m/s" xlink:href="urn:ogc:def:uom:UCUM::m_s"/>
						</swe:Quantity>
					</output>
					<output name="barometricPressure">
						<swe:Quantity definition="urn:ogc:def:property:OGC::BarometricPressure">
							<gml:metaDataProperty>
								<offering>
									<id>ATMOSPHERIC_PRESSURE</id>
									<name>Pressure of the atmosphere</name>
								</offering>
							</gml:metaDataProperty>
							<swe:uom code="hPa" xlink:href="urn:ogc:def:uom:UCUM::hPa"/>
						</swe:Quantity>
					</output>
					<output name="temperature">
						<swe:Quantity definition="urn:ogc:def:property:OGC::Temperature">
							<gml:metaDataProperty>
								<offering>
									<id>ATMOSPHERIC_TEMPERATURE</id>
									<name>Temperature of the atmosphere</name>
								</offering>
							</gml:metaDataProperty>
							<swe:uom code="Cel" xlink:href="urn:ogc:def:uom:UCUM::degC"/>
						</swe:Quantity>
					</output>
					<output name="luminance">
						<swe:Quantity definition="urn:ogc:def:property:OGC::Luminance">
							<gml:metaDataProperty>
								<offering>
									<id>LUMINANCE</id>
									<name>Luminance</name>
								</offering>
							</gml:metaDataProperty>
							<swe:uom code="lx" xlink:href="urn:ogc:def:uom:UCUM::lx"/>
						</swe:Quantity>
					</output>
					<output name="relativeHumidity">
						<swe:Quantity definition="urn:ogc:def:property:OGC::RelativeHumidity">
							<gml:metaDataProperty>
								<offering>
									<id>HUMIDITY</id>
									<name>Humidity of the atmosphere</name>
								</offering>
							</gml:metaDataProperty>
							<swe:uom code="%" xlink:href="urn:ogc:def:uom:UCUM::%25"/>
						</swe:Quantity>
					</output>
				</OutputList>
			</outputs>
			<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->
			<!--Components associated with the System-->
			<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->
			<components>
				<ComponentList>
					<component name="rain-gauge">
						<Component>
							<gml:description>Rain gauge within the weather station located on
								the roof of the Institute for Geoinformatics, University of
								Münster, Germany.</gml:description>
							<keywords>
								<KeywordList>
									<keyword>rain gauge</keyword>
									<keyword>rain</keyword>
									<keyword>precipitation</keyword>
								</KeywordList>
							</keywords>
							<identification>
								<IdentifierList>
									<identifier>
										<Term definition="urn:ogc:def:identifier:OGC:1.0:uniqueID">
											<value>urn:ogc:object:feature:Sensor:OSIRIS-HWS:rain-gauge-3d3b239f-7696-4864-9d07-15447eae2b93</value>
										</Term>
									</identifier>
									<identifier>
										<Term definition="urn:ogc:def:identifier:OGC:1.0:longName">
											<value>OSIRIS Rain-Gauge at weather station IFGI HWS 1</value>
										</Term>
									</identifier>
									<identifier>
										<Term definition="urn:ogc:def:identifier:OGC:1.0:shortName">
											<value>OSIRIS Rain-Gauge IFGI HWS 1</value>
										</Term>
									</identifier>
									<identifier name="productName">
										<Term definition="urn:ogc:def:identifier:OGC:1.0:productName">
											<value>S2000R-1 precipitation sensor</value>
										</Term>
									</identifier>
								</IdentifierList>
							</identification>
							<classification>
								<ClassifierList>
									<classifier name="sensorType">
										<Term definition="urn:ogc:def:classifier:OGC:1.0:sensorType">
											<value>Precipitation</value>
										</Term>
									</classifier>
									<classifier name="intendedApplication">
										<Term definition="urn:ogc:def:classifier:OGC:1.0:application">
											<value>wheather</value>
										</Term>
									</classifier>
								</ClassifierList>
							</classification>
							<capabilities>
								<swe:SimpleDataRecord definition="urn:ogc:def:property:status">
									<swe:field name="status">
										<swe:Text definition="urn:ogc:def:property:OGC:1.0:status">
											<gml:description>The operating status of the sensor.</gml:description>
											<swe:value>active</swe:value>
										</swe:Text>
									</swe:field>
								</swe:SimpleDataRecord>
							</capabilities>
							<contact>
								<ResponsibleParty>
									<organizationName>Institute for Geoinformatics, Münster,
										Germany.</organizationName>
								</ResponsibleParty>
							</contact>
							<position name="rainGaugePosition">
								<swe:Position referenceFrame="#STATION_FRAME">
									<swe:location>
										<swe:Vector>
											<swe:coordinate name="easting">
												<swe:Quantity axisID="x">
													<swe:uom code="m" xlink:href="urn:ogc:def:uom:UCUM::m"/>
													<swe:value>0</swe:value>
												</swe:Quantity>
											</swe:coordinate>
											<swe:coordinate name="northing">
												<swe:Quantity axisID="y">
													<swe:uom code="m" xlink:href="urn:ogc:def:uom:UCUM::m"/>
													<swe:value>0</swe:value>
												</swe:Quantity>
											</swe:coordinate>
											<swe:coordinate name="altitude">
												<swe:Quantity axisID="z">
													<swe:uom code="m" xlink:href="urn:ogc:def:uom:UCUM::m"/>
													<swe:value>0</swe:value>
												</swe:Quantity>
											</swe:coordinate>
										</swe:Vector>
									</swe:location>
								</swe:Position>
							</position>
							<inputs>
								<InputList>
									<input name="precipitation">
										<swe:ObservableProperty definition="urn:ogc:def:property:OGC::Precipitation"/>
									</input>
								</InputList>
							</inputs>
							<outputs>
								<OutputList>
									<output name="precipitation">
										<swe:Quantity definition="urn:ogc:def:property:OGC::Precipitation1Hour">
											<gml:metaDataProperty>
												<offering>
													<id>RAIN_GAUGE</id>
													<name>The rain gauge.</name>
												</offering>
											</gml:metaDataProperty>
											<swe:uom code="mm" xlink:href="urn:ogc:def:uom:UCUM::mm"/>
										</swe:Quantity>
									</output>
								</OutputList>
							</outputs>
						</Component>
					</component>
					<component name="radiometer">
						<Component>
							<gml:description>Radiometer within the weather station located on
								the roof of the Institute for Geoinformatics, University of
								Münster, Germany.</gml:description>
							<keywords>
								<KeywordList>
									<keyword>radiometer</keyword>
									<keyword>luminance</keyword>
								</KeywordList>
							</keywords>
							<identification>
								<IdentifierList>
									<identifier>
										<Term definition="urn:ogc:def:identifier:OGC:1.0:uniqueID">
											<value>urn:ogc:object:feature:Sensor:OSIRIS-HWS:radiometer-3d3b239f-7696-4864-9d07-15447eae2b93</value>
										</Term>
									</identifier>
									<identifier name="longName">
										<Term definition="urn:ogc:def:identifier:OGC:1.0:longName">
											<value>OSIRIS Radiometer at weather station IFGI HWS 1</value>
										</Term>
									</identifier>
									<identifier name="shortName">
										<Term definition="urn:ogc:def:identifier:OGC:1.0:shortName">
											<value>OSIRIS Radiometer IFGI HWS 1</value>
										</Term>
									</identifier>
									<identifier name="productName">
										<Term definition="urn:ogc:def:identifier:OGC:1.0:productName">
											<value>S2500H luminance sensor</value>
										</Term>
									</identifier>
								</IdentifierList>
							</identification>
							<classification>
								<ClassifierList>
									<classifier name="sensorType">
										<Term definition="urn:ogc:def:classifier:OGC:1.0:sensorType">
											<value>radiometer</value>
										</Term>
									</classifier>
									<classifier name="intendedApplication">
										<Term definition="urn:ogc:def:classifier:OGC:1.0:application">
											<value>wheather</value>
										</Term>
									</classifier>
								</ClassifierList>
							</classification>
							<capabilities>
								<swe:SimpleDataRecord definition="urn:ogc:def:property:status">
									<swe:field name="status">
										<swe:Text definition="urn:ogc:def:property:OGC:1.0:status">
											<gml:description>The operating status of the sensor.</gml:description>
											<swe:value>active</swe:value>
										</swe:Text>
									</swe:field>
								</swe:SimpleDataRecord>
							</capabilities>
							<contact>
								<ResponsibleParty>
									<organizationName>Institute for Geoinformatics, Münster,
										Germany.</organizationName>
								</ResponsibleParty>
							</contact>
							<position name="radiometerPosition">
								<swe:Position referenceFrame="#STATION_FRAME">
									<swe:location>
										<swe:Vector>
											<swe:coordinate name="easting">
												<swe:Quantity axisID="x">
													<swe:uom code="m" xlink:href="urn:ogc:def:uom:UCUM::m"/>
													<swe:value>0</swe:value>
												</swe:Quantity>
											</swe:coordinate>
											<swe:coordinate name="northing">
												<swe:Quantity axisID="y">
													<swe:uom code="m" xlink:href="urn:ogc:def:uom:UCUM::m"/>
													<swe:value>0</swe:value>
												</swe:Quantity>
											</swe:coordinate>
											<swe:coordinate name="altitude">
												<swe:Quantity axisID="z">
													<swe:uom code="m" xlink:href="urn:ogc:def:uom:UCUM::m"/>
													<swe:value>0</swe:value>
												</swe:Quantity>
											</swe:coordinate>
										</swe:Vector>
									</swe:location>
								</swe:Position>
							</position>
							<inputs>
								<InputList>
									<input name="luminance">
										<swe:ObservableProperty definition="urn:ogc:def:property:OGC::Luminance"/>
									</input>
								</InputList>
							</inputs>
							<outputs>
								<OutputList>
									<output name="luminance">
										<swe:Quantity definition="urn:ogc:def:property:OGC::Luminance">
											<gml:metaDataProperty>
												<offering>
													<id>LUMINANCE</id>
													<name>The luminance measured.</name>
												</offering>
											</gml:metaDataProperty>
											<swe:uom code="lx" xlink:href="urn:ogc:def:uom:UCUM::lx"/>
										</swe:Quantity>
									</output>
								</OutputList>
							</outputs>
						</Component>
					</component>
					<component name="hygrometer">
						<Component>
							<gml:description>Hygrometer within the weather station located on
								the roof of the Institute for Geoinformatics, University of
								Münster, Germany.</gml:description>
							<keywords>
								<KeywordList>
									<keyword>hygrometer</keyword>
									<keyword>humidity</keyword>
								</KeywordList>
							</keywords>
							<identification>
								<IdentifierList>
									<identifier>
										<Term definition="urn:ogc:def:identifier:OGC:1.0:uniqueID">
											<value>urn:ogc:object:feature:Sensor:OSIRIS-HWS:hygrometer-3d3b239f-7696-4864-9d07-15447eae2b93</value>
										</Term>
									</identifier>
									<identifier name="longName">
										<Term definition="urn:ogc:def:identifier:OGC:1.0:longName">
											<value>OSIRIS Hygrometer at weather station IFGI HWS 1</value>
										</Term>
									</identifier>
									<identifier name="shortName">
										<Term definition="urn:ogc:def:identifier:OGC:1.0:shortName">
											<value>OSIRIS Hygrometer IFGI HWS 1</value>
										</Term>
									</identifier>
									<identifier name="productName">
										<Term definition="urn:ogc:def:identifier:OGC:1.0:productName">
											<value>S2500H humidity sensor</value>
										</Term>
									</identifier>
								</IdentifierList>
							</identification>
							<classification>
								<ClassifierList>
									<classifier name="sensorType">
										<Term definition="urn:ogc:def:classifier:OGC:1.0:sensorType">
											<value>hygrometer</value>
										</Term>
									</classifier>
									<classifier name="intendedApplication">
										<Term definition="urn:ogc:def:classifier:OGC:1.0:application">
											<value>wheather</value>
										</Term>
									</classifier>
								</ClassifierList>
							</classification>
							<capabilities>
								<swe:SimpleDataRecord definition="urn:ogc:def:property:status">
									<swe:field name="status">
										<swe:Text definition="urn:ogc:def:property:OGC:1.0:status">
											<gml:description>The operating status of the sensor.</gml:description>
											<swe:value>active</swe:value>
										</swe:Text>
									</swe:field>
								</swe:SimpleDataRecord>
							</capabilities>
							<contact>
								<ResponsibleParty>
									<organizationName>Institute for Geoinformatics, Münster,
										Germany.</organizationName>
								</ResponsibleParty>
							</contact>
							<position name="hygrometerPosition">
								<swe:Position referenceFrame="#STATION_FRAME">
									<swe:location>
										<swe:Vector>
											<swe:coordinate name="easting">
												<swe:Quantity axisID="x">
													<swe:uom code="m" xlink:href="urn:ogc:def:uom:UCUM::m"/>
													<swe:value>0</swe:value>
												</swe:Quantity>
											</swe:coordinate>
											<swe:coordinate name="northing">
												<swe:Quantity axisID="y">
													<swe:uom code="m" xlink:href="urn:ogc:def:uom:UCUM::m"/>
													<swe:value>0</swe:value>
												</swe:Quantity>
											</swe:coordinate>
											<swe:coordinate name="altitude">
												<swe:Quantity axisID="z">
													<swe:uom code="m" xlink:href="urn:ogc:def:uom:UCUM::m"/>
													<swe:value>0</swe:value>
												</swe:Quantity>
											</swe:coordinate>
										</swe:Vector>
									</swe:location>
								</swe:Position>
							</position>
							<inputs>
								<InputList>
									<input name="humidity">
										<swe:ObservableProperty definition="urn:ogc:def:property:OGC::Humidity"/>
									</input>
								</InputList>
							</inputs>
							<outputs>
								<OutputList>
									<output name="relativeHumidity">
										<swe:Quantity definition="urn:ogc:def:property:OGC::RelativeHumidity">
											<gml:metaDataProperty>
												<offering>
													<id>HUMIDITY</id>
													<name>The relative humidity of the atmosphere.</name>
												</offering>
											</gml:metaDataProperty>
											<swe:uom code="%" xlink:href="urn:ogc:def:uom:UCUM::%25"/>
										</swe:Quantity>
									</output>
								</OutputList>
							</outputs>
						</Component>
					</component>
					<component name="aenometer">
						<Component>
							<gml:description>Aenometer within the weather station located on
								the roof of the Institute for Geoinformatics, University of
								Münster, Germany.</gml:description>
							<keywords>
								<KeywordList>
									<keyword>aenometer</keyword>
									<keyword>wind speed</keyword>
									<keyword>wind</keyword>
								</KeywordList>
							</keywords>
							<identification>
								<IdentifierList>
									<identifier>
										<Term definition="urn:ogc:def:identifier:OGC:1.0:uniqueID">
											<value>urn:ogc:object:feature:Sensor:OSIRIS-HWS:aenometer-3d3b239f-7696-4864-9d07-15447eae2b93</value>
										</Term>
									</identifier>
									<identifier>
										<Term definition="urn:ogc:def:identifier:OGC:1.0:longName">
											<value>OSIRIS Aenometer at weather station IFGI HWS 1</value>
										</Term>
									</identifier>
									<identifier>
										<Term definition="urn:ogc:def:identifier:OGC:1.0:shortName">
											<value>OSIRIS Aenometer IFGI HWS 1</value>
										</Term>
									</identifier>
									<identifier name="productName">
										<Term definition="urn:ogc:def:identifier:OGC:1.0:productName">
											<value>S2000W windsensor</value>
										</Term>
									</identifier>
								</IdentifierList>
							</identification>
							<classification>
								<ClassifierList>
									<classifier name="sensorType">
										<Term definition="urn:ogc:def:classifier:OGC:1.0:sensorType">
											<value>windSpeed</value>
										</Term>
									</classifier>
									<classifier name="sensorType">
										<Term definition="urn:ogc:def:classifier:OGC:1.0:sensorType">
											<value>windDirection</value>
										</Term>
									</classifier>
									<classifier name="intendedApplication">
										<Term definition="urn:ogc:def:classifier:OGC:1.0:application">
											<value>wheather</value>
										</Term>
									</classifier>
								</ClassifierList>
							</classification>
							<capabilities>
								<swe:SimpleDataRecord definition="urn:ogc:def:property:status">
									<swe:field name="status">
										<swe:Text definition="urn:ogc:def:property:OGC:1.0:status">
											<gml:description>The operating status of the sensor.</gml:description>
											<swe:value>active</swe:value>
										</swe:Text>
									</swe:field>
								</swe:SimpleDataRecord>
							</capabilities>
							<contact>
								<ResponsibleParty>
									<organizationName>Institute for Geoinformatics, Münster,
										Germany.</organizationName>
								</ResponsibleParty>
							</contact>
							<position name="aenometerPosition">
								<swe:Position referenceFrame="#STATION_FRAME">
									<swe:location>
										<swe:Vector>
											<swe:coordinate name="easting">
												<swe:Quantity axisID="x">
													<swe:uom code="m" xlink:href="urn:ogc:def:uom:UCUM::m"/>
													<swe:value>0</swe:value>
												</swe:Quantity>
											</swe:coordinate>
											<swe:coordinate name="northing">
												<swe:Quantity axisID="y">
													<swe:uom code="m" xlink:href="urn:ogc:def:uom:UCUM::m"/>
													<swe:value>0</swe:value>
												</swe:Quantity>
											</swe:coordinate>
											<swe:coordinate name="altitude">
												<swe:Quantity axisID="z">
													<swe:uom code="m" xlink:href="urn:ogc:def:uom:UCUM::m"/>
													<swe:value>0</swe:value>
												</swe:Quantity>
											</swe:coordinate>
										</swe:Vector>
									</swe:location>
								</swe:Position>
							</position>
							<inputs>
								<InputList>
									<input name="wind">
										<swe:ObservableProperty definition="urn:ogc:def:property:OGC::Wind"/>
									</input>
								</InputList>
							</inputs>
							<outputs>
								<OutputList>
									<output name="windSpeed">
										<swe:Quantity definition="urn:ogc:def:property:OGC::WindSpeed">
											<gml:metaDataProperty>
												<offering>
													<id>WIND_SPEED</id>
													<name>The speed of the measured wind.</name>
												</offering>
											</gml:metaDataProperty>
											<swe:uom code="m/s" xlink:href="urn:ogc:def:uom:UCUM::m_s"/>
										</swe:Quantity>
									</output>
									<output name="windDirection">
										<swe:Quantity definition="urn:ogc:def:property:OGC::WindDirection">
											<gml:metaDataProperty>
												<offering>
													<id>WIND_DIRECTION</id>
													<name>The direction of the measured wind.</name>
												</offering>
											</gml:metaDataProperty>
											<swe:uom code="deg" xlink:href="urn:ogc:def:uom:UCUM::deg"/>
										</swe:Quantity>
									</output>
								</OutputList>
							</outputs>
						</Component>
					</component>
					<component name="barmometer">
						<Component>
							<gml:description>Barometer within the weather station located on
								the roof of the Institute for Geoinformatics, University of
								Münster, Germany.</gml:description>
							<keywords>
								<KeywordList>
									<keyword>barometer</keyword>
									<keyword>barometric pressure</keyword>
								</KeywordList>
							</keywords>
							<identification>
								<IdentifierList>
									<identifier>
										<Term definition="urn:ogc:def:identifier:OGC:1.0:uniqueID">
											<value>urn:ogc:object:feature:Sensor:OSIRIS-HWS:barometer-3d3b239f-7696-4864-9d07-15447eae2b93</value>
										</Term>
									</identifier>
									<identifier name="longName">
										<Term definition="urn:ogc:def:identifier:OGC:1.0:longName">
											<value>OSIRIS Barometer at weather station IFGI HWS 1</value>
										</Term>
									</identifier>
									<identifier name="shortName">
										<Term definition="urn:ogc:def:identifier:OGC:1.0:shortName">
											<value>OSIRIS Barometer IFGI HWS 1</value>
										</Term>
									</identifier>
									<identifier name="productName">
										<Term definition="urn:ogc:def:identifier:OGC:1.0:productName">
											<value>S2000B pressure sensor</value>
										</Term>
									</identifier>
								</IdentifierList>
							</identification>
							<classification>
								<ClassifierList>
									<classifier name="sensorType">
										<Term definition="urn:ogc:def:classifier:OGC:1.0:sensorType">
											<value>barometer</value>
										</Term>
									</classifier>
									<classifier name="intendedApplication">
										<Term definition="urn:ogc:def:classifier:OGC:1.0:application">
											<value>wheather</value>
										</Term>
									</classifier>
								</ClassifierList>
							</classification>
							<capabilities>
								<swe:SimpleDataRecord definition="urn:ogc:def:property:status">
									<swe:field name="status">
										<swe:Text definition="urn:ogc:def:property:OGC:1.0:status">
											<gml:description>The operating status of the sensor.</gml:description>
											<swe:value>active</swe:value>
										</swe:Text>
									</swe:field>
								</swe:SimpleDataRecord>
							</capabilities>
							<contact>
								<ResponsibleParty>
									<organizationName>Institute for Geoinformatics, Münster,
										Germany.</organizationName>
								</ResponsibleParty>
							</contact>
							<position name="thermometerPosition">
								<swe:Position referenceFrame="#STATION_FRAME">
									<swe:location>
										<swe:Vector>
											<swe:coordinate name="easting">
												<swe:Quantity axisID="x">
													<swe:uom code="m" xlink:href="urn:ogc:def:uom:UCUM::m"/>
													<swe:value>0</swe:value>
												</swe:Quantity>
											</swe:coordinate>
											<swe:coordinate name="northing">
												<swe:Quantity axisID="y">
													<swe:uom code="m" xlink:href="urn:ogc:def:uom:UCUM::m"/>
													<swe:value>0</swe:value>
												</swe:Quantity>
											</swe:coordinate>
											<swe:coordinate name="altitude">
												<swe:Quantity axisID="z">
													<swe:uom code="m" xlink:href="urn:ogc:def:uom:UCUM::m"/>
													<swe:value>0</swe:value>
												</swe:Quantity>
											</swe:coordinate>
										</swe:Vector>
									</swe:location>
								</swe:Position>
							</position>
							<inputs>
								<InputList>
									<input name="atmosphericPressure">
										<swe:ObservableProperty definition="urn:ogc:def:property:OGC::AtmospericPressure"/>
									</input>
								</InputList>
							</inputs>
							<outputs>
								<OutputList>
									<output name="barometricPressure">
										<swe:Quantity definition="urn:ogc:def:property:OGC::BarometricPressure">
											<gml:metaDataProperty>
												<offering>
													<id>ATMOSPHERIC_PRESSURE</id>
													<name>The pressure of the atmosphere.</name>
												</offering>
											</gml:metaDataProperty>
											<swe:uom code="hPa" xlink:href="urn:ogc:def:uom:UCUM::hPa"/>
										</swe:Quantity>
									</output>
								</OutputList>
							</outputs>
						</Component>
					</component>
					<component name="thermometer">
						<Component>
							<gml:description>Thermometer within the weather station located
								on the roof of the Institute for Geoinformatics, University of
								Münster, Germany.</gml:description>
							<keywords>
								<KeywordList>
									<keyword>thermometer</keyword>
									<keyword>temperature</keyword>
								</KeywordList>
							</keywords>
							<identification>
								<IdentifierList>
									<identifier>
										<Term definition="urn:ogc:def:identifier:OGC:1.0:uniqueID">
											<value>urn:ogc:object:feature:Sensor:OSIRIS-HWS:thermometer-3d3b239f-7696-4864-9d07-15447eae2b93</value>
										</Term>
									</identifier>
									<identifier name="longName">
										<Term definition="urn:ogc:def:identifier:OGC:1.0:longName">
											<value>OSIRIS Thermometer at weather station IFGI HWS 1</value>
										</Term>
									</identifier>
									<identifier name="shortName">
										<Term definition="urn:ogc:def:identifier:OGC:1.0:shortName">
											<value>OSIRIS Thermometer IFGI HWS 1</value>
										</Term>
									</identifier>
									<identifier name="productName">
										<Term definition="urn:ogc:def:identifier:OGC:1.0:productName">
											<value>S2001IA temperature sensor</value>
										</Term>
									</identifier>
								</IdentifierList>
							</identification>
							<classification>
								<ClassifierList>
									<classifier name="sensorType">
										<Term definition="urn:ogc:def:classifier:OGC:1.0:sensorType">
											<value>thermometer</value>
										</Term>
									</classifier>
									<classifier name="intendedApplication">
										<Term definition="urn:ogc:def:classifier:OGC:1.0:application">
											<value>wheather</value>
										</Term>
									</classifier>
								</ClassifierList>
							</classification>
							<capabilities>
								<swe:SimpleDataRecord definition="urn:ogc:def:property:status">
									<swe:field name="status">
										<swe:Text definition="urn:ogc:def:property:OGC:1.0:status">
											<gml:description>The operating status of the sensor.</gml:description>
											<swe:value>active</swe:value>
										</swe:Text>
									</swe:field>
								</swe:SimpleDataRecord>
							</capabilities>
							<contact>
								<ResponsibleParty>
									<organizationName>Institute for Geoinformatics, Münster,
										Germany.</organizationName>
								</ResponsibleParty>
							</contact>
							<position name="thermometerPosition">
								<swe:Position referenceFrame="#STATION_FRAME">
									<swe:location>
										<swe:Vector>
											<swe:coordinate name="easting">
												<swe:Quantity axisID="x">
													<swe:uom code="m" xlink:href="urn:ogc:def:uom:UCUM::m"/>
													<swe:value>0</swe:value>
												</swe:Quantity>
											</swe:coordinate>
											<swe:coordinate name="northing">
												<swe:Quantity axisID="y">
													<swe:uom code="m" xlink:href="urn:ogc:def:uom:UCUM::m"/>
													<swe:value>0</swe:value>
												</swe:Quantity>
											</swe:coordinate>
											<swe:coordinate name="altitude">
												<swe:Quantity axisID="z">
													<swe:uom code="m" xlink:href="urn:ogc:def:uom:UCUM::m"/>
													<swe:value>0</swe:value>
												</swe:Quantity>
											</swe:coordinate>
										</swe:Vector>
									</swe:location>
								</swe:Position>
							</position>
							<inputs>
								<InputList>
									<input name="atmosphericTemperature">
										<swe:ObservableProperty definition="urn:ogc:def:property:OGC::AirTemperature"/>
									</input>
								</InputList>
							</inputs>
							<outputs>
								<OutputList>
									<output name="temperature">
										<swe:Quantity definition="urn:ogc:def:property:OGC::Temperature">
											<gml:metaDataProperty>
												<offering>
													<id>ATMOSPHERIC_TEMPERATURE</id>
													<name>Temperature of the atmosphere.</name>
												</offering>
											</gml:metaDataProperty>
											<swe:uom code="Cel" xlink:href="urn:ogc:def:uom:UCUM::degC"/>
										</swe:Quantity>
									</output>
								</OutputList>
							</outputs>
						</Component>
					</component>
				</ComponentList>
			</components>
		</System>
	</member>
</SensorML>
