Ksat {geoR} | R Documentation

## Saturated Hydraulic Conductivity

### Description

The data consists of 32 measurements of the saturated hydraulic conductivity of a soil.

### Usage

    data(Ksat)

### Format

The object `Ksat` is a list of the class `geodata` with the following elements:

`coords`
  a matrix with the coordinates of the soil samples.
`data`
  measurements of the saturated hidraulic conductivity.
`borders`
  a data-frame with the coordinates of a polygon defining the borders of the area.

### Source

Data provided by Dr. Décio Cruciani, ESALQ/USP, Brasil.

### Examples

    summary(Ksat)
    plot(Ksat, border=borders)

[Package geoR version 1.6-19 Index]