ztex_inouttraffic Project Status (06/28/2017 - 11:38:33)
Project File: | descrypt-ztex.xise | Parser Errors: | No Errors
Module Name: | ztex_inouttraffic | Implementation State: | Programming File Generated
Target Device: | xc6slx150-3csg484 | Errors: |
Product Version: | ISE 14.5 | Warnings: |
Design Goal: | Balanced | Routing Results: | All Signals Completely Routed
Design Strategy: | descrypt | Timing Constraints: | All Constraints Met
Environment: | System Settings | Final Timing Score: | 0 (Timing Report)

Device Utilization Summary | [-]
Slice Logic Utilization | Used | Available | Utilization | Note(s)
Number of Slice Registers | 53,703 | 184,304 | 29% |
Number used as Flip Flops | 53,675 |  |  |
Number used as Latches | 28 |  |  |
Number used as Latch-thrus | 0 |  |  |
Number used as AND/OR logics | 0 |  |  |
Number of Slice LUTs | 53,817 | 92,152 | 58% |
Number used as logic | 44,476 | 92,152 | 48% |
Number using O6 output only | 36,628 |  |  |
Number using O5 output only | 156 |  |  |
Number using O5 and O6 | 7,692 |  |  |
Number used as ROM | 0 |  |  |
Number used as Memory | 2,220 | 21,680 | 10% |
Number used as Dual Port RAM | 744 |  |  |
Number using O6 output only | 40 |  |  |
Number using O5 output only | 0 |  |  |
Number using O5 and O6 | 704 |  |  |
Number used as Single Port RAM | 104 |  |  |
Number using O6 output only | 104 |  |  |
Number using O5 output only | 0 |  |  |
Number using O5 and O6 | 0 |  |  |
Number used as Shift Register | 1,372 |  |  |
Number using O6 output only | 27 |  |  |
Number using O5 output only | 0 |  |  |
Number using O5 and O6 | 1,345 |  |  |
Number used exclusively as route-thrus | 7,121 |  |  |
Number with same-slice register load | 7,111 |  |  |
Number with same-slice carry load | 10 |  |  |
Number with other load | 0 |  |  |
Number of occupied Slices | 15,823 | 23,038 | 68% |
Number of MUXCYs used | 1,684 | 46,076 | 3% |
Number of LUT Flip Flop pairs used | 58,562 |  |  |
Number with an unused Flip Flop | 17,921 | 58,562 | 30% |
Number with an unused LUT | 4,745 | 58,562 | 8% |
Number of fully used LUT-FF pairs | 35,896 | 58,562 | 61% |
Number of unique control sets | 566 |  |  |
Number of slice register sites lost to control set restrictions | 2,244 | 184,304 | 1% |
Number of bonded IOBs | 44 | 338 | 13% |
Number of LOCed IOBs | 44 | 44 | 100% |
IOB Flip Flops | 62 |  |  |
Number of RAMB16BWERs | 134 | 268 | 50% |
Number of RAMB8BWERs | 6 | 536 | 1% |
Number of BUFIO2/BUFIO2_2CLKs | 1 | 32 | 3% |
Number used as BUFIO2s | 1 |  |  |
Number used as BUFIO2_2CLKs | 0 |  |  |
Number of BUFIO2FB/BUFIO2FB_2CLKs | 1 | 32 | 3% |
Number used as BUFIO2FBs | 1 |  |  |
Number used as BUFIO2FB_2CLKs | 0 |  |  |
Number of BUFG/BUFGMUXs | 7 | 16 | 43% |
Number used as BUFGs | 5 |  |  |
Number used as BUFGMUX | 2 |  |  |
Number of DCM/DCM_CLKGENs | 3 | 12 | 25% |
Number used as DCMs | 1 |  |  |
Number used as DCM_CLKGENs | 2 |  |  |
Number of ILOGIC2/ISERDES2s | 20 | 586 | 3% |
Number used as ILOGIC2s | 20 |  |  |
Number used as ISERDES2s | 0 |  |  |
Number of IODELAY2/IODRP2/IODRP2_MCBs | 0 | 586 | 0% |
Number of OLOGIC2/OSERDES2s | 22 | 586 | 3% |
Number used as OLOGIC2s | 22 |  |  |
Number used as OSERDES2s | 0 |  |  |
Number of BSCANs | 0 | 4 | 0% |
Number of BUFHs | 0 | 384 | 0% |
Number of BUFPLLs | 0 | 8 | 0% |
Number of BUFPLL_MCBs | 0 | 4 | 0% |
Number of DSP48A1s | 1 | 180 | 1% |
Number of ICAPs | 0 | 1 | 0% |
Number of MCBs | 0 | 4 | 0% |
Number of PCILOGICSEs | 0 | 2 | 0% |
Number of PLL_ADVs | 3 | 6 | 50% |
Number of LOCed PLL_ADVs | 3 | 3 | 100% |
Number of PMVs | 0 | 1 | 0% |
Number of STARTUPs | 1 | 1 | 100% |
Number of SUSPEND_SYNCs | 0 | 1 | 0% |
Average Fanout of Non-Clock Nets | 2.60 |  |  |

Performance Summary | [-]
Final Timing Score: | 0 (Setup: 0, Hold: 0, Component Switching Limit: 0) | Pinout Data: | Pinout Report
Routing Results: | All Signals Completely Routed | Clock Data: | Clock Report
Timing Constraints: | All Constraints Met |  |

Detailed Reports | [-]
Report Name | Status | Generated | Errors | Warnings | Infos
Synthesis Report | Current | Âò 27. èþí 23:23:55 2017 | 0 | 110 Warnings (110 new) | 32 Infos (32 new)
Translation Report | Current | Ñð 28. èþí 05:58:30 2017 | 0 | 2 Warnings (2 new) | 2 Infos (2 new)
Map Report | Current | Ñð 28. èþí 07:05:24 2017 |  |  |
Place and Route Report | Current | Ñð 28. èþí 08:29:31 2017 | 0 | 186 Warnings (186 new) | 1 Info (1 new)
Power Report |  |  |  |  |
Post-PAR Static Timing Report | Current | Ñð 28. èþí 11:38:11 2017 | 0 | 2 Warnings (0 new) | 3 Infos (0 new)
Bitgen Report | Current | Ñð 28. èþí 09:02:31 2017 | 0 | 209 Warnings (209 new) | 1 Info (1 new)

Secondary Reports | [-]
Report Name | Status | Generated
WebTalk Log File | Current | Ñð 28. èþí 09:03:13 2017

Date Generated: 06/28/2017 - 11:38:33