ztex_inouttraffic Project Status (02/21/2019 - 15:06:53)
Project File: | fpga-bcrypt-ztex.xise | Parser Errors: | No Errors
Module Name: | ztex_inouttraffic | Implementation State: | Programming File Generated
Target Device: | xc6slx150-3csg484 | Errors: |
Product Version: | ISE 14.5 | Warnings: |
Design Goal: | Balanced | Routing Results: | All Signals Completely Routed
Design Strategy: | bcrypt | Timing Constraints: | X 1 Failing Constraint
Environment: | System Settings | Final Timing Score: | 1109 (Timing Report)

Device Utilization Summary | [-]
Slice Logic Utilization | Used | Available | Utilization | Note(s)
Number of Slice Registers | 30,064 | 184,304 | 16% |
Number used as Flip Flops | 30,064 |  |  |
Number used as Latches | 0 |  |  |
Number used as Latch-thrus | 0 |  |  |
Number used as AND/OR logics | 0 |  |  |
Number of Slice LUTs | 51,258 | 92,152 | 55% |
Number used as logic | 44,294 | 92,152 | 48% |
Number using O6 output only | 34,146 |  |  |
Number using O5 output only | 1,298 |  |  |
Number using O5 and O6 | 8,850 |  |  |
Number used as ROM | 0 |  |  |
Number used as Memory | 6,101 | 21,680 | 28% |
Number used as Dual Port RAM | 3,598 |  |  |
Number using O6 output only | 1,010 |  |  |
Number using O5 output only | 44 |  |  |
Number using O5 and O6 | 2,544 |  |  |
Number used as Single Port RAM | 2,502 |  |  |
Number using O6 output only | 17 |  |  |
Number using O5 output only | 3 |  |  |
Number using O5 and O6 | 2,482 |  |  |
Number used as Shift Register | 1 |  |  |
Number using O6 output only | 1 |  |  |
Number using O5 output only | 0 |  |  |
Number using O5 and O6 | 0 |  |  |
Number used exclusively as route-thrus | 863 |  |  |
Number with same-slice register load | 713 |  |  |
Number with same-slice carry load | 150 |  |  |
Number with other load | 0 |  |  |
Number of occupied Slices | 17,232 | 23,038 | 74% |
Number of MUXCYs used | 12,600 | 46,076 | 27% |
Number of LUT Flip Flop pairs used | 57,302 |  |  |
Number with an unused Flip Flop | 29,599 | 57,302 | 51% |
Number with an unused LUT | 6,044 | 57,302 | 10% |
Number of fully used LUT-FF pairs | 21,659 | 57,302 | 37% |
Number of unique control sets | 2,967 |  |  |
Number of slice register sites lost to control set restrictions | 10,209 | 184,304 | 5% |
Number of bonded IOBs | 44 | 338 | 13% |
Number of LOCed IOBs | 44 | 44 | 100% |
IOB Flip Flops | 58 |  |  |
Number of RAMB16BWERs | 10 | 268 | 3% |
Number of RAMB8BWERs | 497 | 536 | 92% |
Number of BUFIO2/BUFIO2_2CLKs | 1 | 32 | 3% |
Number used as BUFIO2s | 1 |  |  |
Number used as BUFIO2_2CLKs | 0 |  |  |
Number of BUFIO2FB/BUFIO2FB_2CLKs | 1 | 32 | 3% |
Number used as BUFIO2FBs | 1 |  |  |
Number used as BUFIO2FB_2CLKs | 0 |  |  |
Number of BUFG/BUFGMUXs | 3 | 16 | 18% |
Number used as BUFGs | 2 |  |  |
Number used as BUFGMUX | 1 |  |  |
Number of DCM/DCM_CLKGENs | 2 | 12 | 16% |
Number used as DCMs | 1 |  |  |
Number used as DCM_CLKGENs | 1 |  |  |
Number of ILOGIC2/ISERDES2s | 20 | 586 | 3% |
Number used as ILOGIC2s | 20 |  |  |
Number used as ISERDES2s | 0 |  |  |
Number of IODELAY2/IODRP2/IODRP2_MCBs | 0 | 586 | 0% |
Number of OLOGIC2/OSERDES2s | 22 | 586 | 3% |
Number used as OLOGIC2s | 22 |  |  |
Number used as OSERDES2s | 0 |  |  |
Number of BSCANs | 0 | 4 | 0% |
Number of BUFHs | 0 | 384 | 0% |
Number of BUFPLLs | 0 | 8 | 0% |
Number of BUFPLL_MCBs | 0 | 4 | 0% |
Number of DSP48A1s | 1 | 180 | 1% |
Number of ICAPs | 0 | 1 | 0% |
Number of MCBs | 0 | 4 | 0% |
Number of PCILOGICSEs | 0 | 2 | 0% |
Number of PLL_ADVs | 1 | 6 | 16% |
Number of LOCed PLL_ADVs | 1 | 1 | 100% |
Number of PMVs | 0 | 1 | 0% |
Number of STARTUPs | 1 | 1 | 100% |
Number of SUSPEND_SYNCs | 0 | 1 | 0% |
Average Fanout of Non-Clock Nets | 3.61 |  |  |

Performance Summary | [-]
Final Timing Score: | 1109 (Setup: 1109, Hold: 0, Component Switching Limit: 0) | Pinout Data: | Pinout Report
Routing Results: | All Signals Completely Routed | Clock Data: | Clock Report
Timing Constraints: | X 1 Failing Constraint |  |

Detailed Reports | [-]
Report Name | Status | Generated | Errors | Warnings | Infos
Synthesis Report | Current | Чт 21. фев 14:21:22 2019 | 0 | 130 Warnings (1 new) | 9 Infos (0 new)
Translation Report | Current | Чт 21. фев 14:25:50 2019 | 0 | 0 | 0
Map Report | Current | Чт 21. фев 14:44:53 2019 |  |  |
Place and Route Report | Current | Чт 21. фев 14:57:36 2019 | 0 | 1277 Warnings (1277 new) | 2 Infos (2 new)
Power Report |  |  |  |  |
Post-PAR Static Timing Report | Current | Чт 21. фев 14:58:53 2019 | 0 | 1 Warning (1 new) | 4 Infos (4 new)
Bitgen Report | Current | Чт 21. фев 15:06:48 2019 | 0 | 1268 Warnings (1268 new) | 1 Info (1 new)

Secondary Reports | [-]
Report Name | Status | Generated
WebTalk Log File | Current | Чт 21. фев 15:06:49 2019

Date Generated: 02/21/2019 - 15:06:54