linenr
Prev | Orchestra Opcodes and Operators | Next

## linenr

linenr — The linen opcode extended with a final release segment.

## Description

linenr -- same as linen except that the final segment is entered only on sensing a MIDI note release. The note is then extended by the decay time.

## Syntax

    ares linenr xamp, irise, idec, iatdec

    kres linenr kamp, irise, idec, iatdec

## Initialization

irise -- rise time in seconds. A zero or negative value signifies no rise modification.

idec -- decay time in seconds. Zero means no decay. An idec > idur will cause a truncated decay.

iatdec -- attenuation factor by which the closing steady state value is reduced exponentially over the decay period. This value must be positive and is normally of the order of .01. A large or excessively small value is apt to produce a cutoff which is audible. A zero or negative value is illegal.

## Performance

kamp, xamp -- input amplitude signal.

linenr is unique within Csound in containing a note-off sensor and release time extender. When it senses either a score event termination or a MIDI noteoff, it will immediately extend the performance time of the current instrument by idec seconds, then execute an exponential decay towards the factor iatdec. For two or more units in an instrument, extension is by the greatest idec.

You can use other pre-made envelopes which start a release segment upon receiving a note off message, like linsegr and expsegr, or you can construct more complex envelopes using xtratim and release. Note that you don't need to use xtratim if you are using linenr, since the time is extended automatically.

These “r” units can also be modified by MIDI noteoff velocities (see veloffs).

## Examples

Here is an example of the linenr opcode. It uses the file linenr.csd.

Example 422. Example of the linenr opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    ; Audio out   Audio in
    -odac           -iadc       -M0 ;;;RT audio I/O with MIDI in
    </CsOptions>
    <CsInstruments>

    ; Example by Jonathan Murphy and Charles Gran 2007
      sr	    =  44100
      ksmps	    =  10
      nchnls    =  2

            ; new, and important. Make sure that midi note events are only
            ; received by instruments that actually need them.

    	; turn default midi routing off
    	massign		0, 0
    	; route note events on channel 1 to instr 1
    	massign		1, 1

    ; Define your midi controllers
    #define C1 #21#
    #define C2 #22#
    #define C3 #23#

    ; Initialize MIDI controllers
    	    initc7    1, 21, 0.5 		  ;delay send
    	    initc7    1, 22, 0.5		  ;delay: time to zero
    	    initc7    1, 23, 0.5 		  ;delay: rate

      gaosc	    init      0

    ; Define an opcode to "smooth" the MIDI controller signal
        opcode smooth, k, k
      kin       xin
      kport	    linseg    0, 0.0001, 0.01, 1, 0.01
      kin       portk     kin, kport
                xout      kin
        endop

    instr   1
     ; Generate a sine wave at the frequency of the MIDI note that triggered the intrument
      ifqc	    cpsmidi
      iamp	    ampmidi   10000
      aenv	    linenr    iamp, .01, .1, .01 	  ;envelope
      a1	    oscil     aenv, ifqc, 1
    ; All sound goes to the global variable gaosc
      gaosc	    =  gaosc + a1
        endin

        instr     198 ; ECHO
      kcmbsnd   ctrl7     1, 21, 0, 1 		  ;delay send
      ktime	    ctrl7     1, 22, 0.01, 6 		  ;time loop fades out
      kloop	    ctrl7     1, 23, 0.01, 1 		  ;loop speed
    ; Receive MIDI controller values and then smooth them
      kcmbsnd   smooth    kcmbsnd
      ktime	    smooth    ktime
      kloop	    smooth    kloop

      imaxlpt   =  1 				  ;max loop time
    ; Create a variable reverberation (delay) of the gaosc signal
      acomb	    vcomb     gaosc, ktime, kloop, imaxlpt, 1
      aout	    =  (acomb * kcmbsnd) + gaosc * (1 - kcmbsnd)
    	    outs      aout, aout
      gaosc	    =  0
        endin

    </CsInstruments>
    <CsScore>
    f1 0 16384 10 1
    i198 0 10000
    e
    </CsScore>
    </CsoundSynthesizer>

## See Also

linsegr, expsegr, envlpxr, mxadsr, madsr, envlpx, linen, xtratim

Prev | Up | Next
linen | Home | lineto