vbap4move
Prev | Orchestra Opcodes and Operators | Next

## vbap4move

vbap4move — Distributes an audio signal among 4 channels with moving virtual sources.

## Description

Distributes an audio signal among 4 channels with moving virtual sources.

## Syntax

    ar1, ar2, ar3, ar4 vbap4move asig, idur, ispread, ifldnum, ifld1 \
          [, ifld2] [...]

## Initialization

idur -- the duration over which the movement takes place.

ispread -- spreading of the virtual source (range 0 - 100). If value is zero, conventional amplitude panning is used. When ispread is increased, the number of loudspeakers used in panning increases. If value is 100, the sound is applied to all loudspeakers.

ifldnum -- number of fields (absolute value must be 2 or larger). If ifldnum is positive, the virtual source movement is a polyline specified by given directions. Each transition is performed in an equal time interval. If ifldnum is negative, specified angular velocities are applied to the virtual source during specified relative time intervals (see below).

ifld1, ifld2, ... -- azimuth angles or angular velocities, and relative durations of movement phases (see below).

## Performance

asig -- audio signal to be panned

vbap4move allows the use of moving virtual sources. If ifldnum is positive, the fields represent directions of virtual sources and equal times, iazi1, [iele1,] iazi2, [iele2,], etc. The position of the virtual source is interpolated between directions starting from the first direction and ending at the last. Each interval is interpolated in time that is fraction total_time / number_of_intervals of the duration of the sound event.

If ifldnum is negative, the fields represent angular velocities and equal times. The first field is, however, the starting direction, iazi1, [iele1,] iazi_vel1, [iele_vel1,] iazi_vel2, [iele_vel2,] .... Each velocity is applied to the note that is fraction total_time / number_of_velocities of the duration of the sound event. If the elevation of the virtual source becomes greater than 90 degrees or less than 0 degrees, the polarity of angular velocity is changed. Thus the elevational angular velocity produces a virtual source that moves up and down between 0 and 90 degrees.

| Warning
Please note that all vbap panning opcodes require the vbap system to be initialized using vbaplsinit.

## Examples

See the entry for vbap8move for an example of usage of the vbapXmove opcodes.

## Reference

Ville Pulkki: “Virtual Sound Source Positioning Using Vector Base Amplitude Panning” Journal of the Audio Engineering Society, 1997 June, Vol. 45/6, p. 456.

## Examples

Here is an example of the vbap4move opcode. It uses the file vbap4move.csd.

Example 977. Example of the vbap4move opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac  ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o vbap4move.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 4	;quad
    0dbfs  = 1

    vbaplsinit 2, 4, 0, 90, 180, 270

    instr 1

    asig diskin2 "beats.wav", 1, 0, 1		;loop beats.wav
    a1,a2,a3,a4 vbap4move  asig, p3, 1, 2, 310, 180	;change movement of soundsource in
         outq a1,a2,a3,a4				;the rear speakers

    endin
    </CsInstruments>
    <CsScore>

    i 1 0 5

    e
    </CsScore>
    </CsoundSynthesizer>

## See Also

vbap16, vbap16move, vbap4, vbap8, vbap8move, vbaplsinit, vbapz, vbapzmove

## Credits

Author: Ville Pulkki
Sibelius Academy Computer Music Studio
Laboratory of Acoustics and Audio Signal Processing
Helsinki University of Technology
Helsinki, Finland
May 2000

New in Csound Version 4.07

Prev | Up | Next
vbap4 | Home | vbap8