jitter
Prev | Orchestra Opcodes and Operators | Next

## jitter

jitter — Generates a segmented line whose segments are randomly generated.

## Description

Generates a segmented line whose segments are randomly generated.

## Syntax

    kout jitter kamp, kcpsMin, kcpsMax

## Performance

kamp -- Amplitude of jitter deviation

kcpsMin -- Minimum speed of random frequency variations (expressed in cps)

kcpsMax -- Maximum speed of random frequency variations (expressed in cps)

jitter generates a segmented line whose segments are randomly generated inside the +kamp and -kamp interval. Duration of each segment is a random value generated according to kcpsmin and kcpsmax values.

jitter can be used to make more natural and “analog-sounding” some static, dull sound. For best results, it is suggested to keep its amplitude moderate.

## Examples

Here is an example of the jitter opcode. It uses the file jitter.csd.

Example 413. Example of the jitter opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac     ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o jitter.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    instr 1

    kamp    init p4
    kcpsmin init 4
    kcpsmax init 8

    kj2  jitter kamp, kcpsmin, kcpsmax
    aout pluck 1, 200+kj2, 1000, 0, 1
    aout dcblock aout	;remove DC
         outs aout, aout

    endin
    </CsInstruments>
    <CsScore>

    i 1 0 15 2	;a bit jitter
    i 1 8 15 10	;some more
    i 1 16 15 20	;lots more
    e
    </CsScore>
    </CsoundSynthesizer>

## See Also

jitter2, vibr, vibrato

## Credits

Author: Gabriel Maldonado

New in Version 4.15

Prev | Up | Next
jacktransport | Home | jitter2