chano
Prev | Orchestra Opcodes and Operators | Next

## chano

chano — Send data to the outwards software bus

## Description

Send data to a channel of the outward software bus.

## Syntax

    chano kval, kchan

    chano aval, kchan

## Performance

xval --- value to transmit

kchan -- a positive integer that indicates which channel of the software bus to write

Note that the inward and outward software busses are independent, and are not mixer buses. Also the k-rate and a-rate busses are independent. The last value remains until a new value is written. There is no imposed limit to the number of busses but they use memory so small numbers are to be preferred.

## Example

The example shows the software bus being used as an output audio channel. It assumes that an external program that has access to the API is receiving the values.

            sr = 44100
            kr = 100
            ksmps = 1

            instr   1
               a1   oscil     p4, p5, 100
                    chano     1, a1
            endin

## Credits

Author: John ffitch
2005

New in Csound 5.00

Prev | Up | Next
chani | Home | chebyshevpoly