biquada
Prev | Orchestra Opcodes and Operators | Next

## biquada

biquada — A sweepable general purpose biquadratic digital filter with a-rate parameters.

## Description

A sweepable general purpose biquadratic digital filter.

## Syntax

    ares biquada asig, ab0, ab1, ab2, aa0, aa1, aa2 [, iskip]

## Initialization

iskip (optional, default=0) -- if non-zero, intialization will be skipped. Default value 0. (New in Csound version 3.50)

## Performance

asig -- input signal

biquada is a general purpose biquadratic digital filter of the form:

a0*y(n) + a1*y[n-1] + a2*y[n-2] = b0*x[n] + b1*x[n-1] + b2*x[n-2]

This filter has the following frequency response:

B(Z) b0 + b1*Z-1 + b2*Z-2
H(Z) = ---- = ------------------
A(Z) a0 + a1*Z-1 + a2*Z-2

This type of filter is often encountered in digital signal processing literature. It allows six user-defined a-rate coefficients.

## See Also

biquad

## Credits

Author: Hans Mikelson
October 1998

New in Csound version 3.49

Prev | Up | Next
biquad | Home | birnd