partikkelsync
Précédent | Opcodes et opérateurs de l'orchestre | Suivant

## partikkelsync

partikkelsync — Produit l'impulsion et la phase de l'horloge du distributeur de grain de partikkel pour synchroniser plusieurs instances de l'opcode partikkel à la même source d'horloge.

## Description

partikkelsync est un opcode dont la tâche est de produire l'impulsion et la phase de l'horloge du distributeur de grain de partikkel. On peut utiliser la sortie de partikkelsync pour synchroniser d'autres instances de l'opcode partikkel à la même horloge.

## Syntaxe

    async [,aphase] partikkelsync iopcode_id

## Initialisation

iopcode_id -- identificateur de l'opcode, liant une instance de partikkel à une instance de partikkelsync.

## Exécution

async -- signal d'impulsion de déclenchement. Envoie des impulsions de déclenchement synchronisées à l'horloge du distributeur de grain d'un opcode partikkel. Une impulsion de déclenchement est générée pour le démarrage de chaque grain dans l'opcode partikkel ayant le même opcode_id. Dans une utilisation normale, on enverra ce signal à l'entrée async d'un autre opcode partikkel pour synchroniser plusieurs instances de partikkel.

aphase -- phase de l'horloge. Sort un signal de phase linéaire. On peut l'utiliser par exemple pour une synchronisation légère, ou simplement comme un générateur de phase à la phasor.

## Exemples

Voici un exemple de l'opcode partikkelsync. Il utilise le fichier partikkelsync.csd.

Exemple 629. Exemple de l'opcode partikkelsync.

Voir les sections Audio en Temps Réel et Options de la Ligne de Commande pour plus d'information sur l'utilisation des options de la ligne de commande.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    ; Audio out
    -odac           ;;;RT audio
    ; For Non-realtime ouput leave only the line below:
    ; -o partikkel_softsync.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 20
    nchnls = 2

    ; Example by Oeyvind Brandtsegg 2007, revised 2008

    giSine		ftgen	0, 0, 65537, 10, 1
    giCosine	ftgen	0, 0, 8193, 9, 1, 1, 90
    giSigmoRise	ftgen		0, 0, 8193, 19, 0.5, 1, 270, 1			; rising sigmoid
    giSigmoFall	ftgen		0, 0, 8193, 19, 0.5, 1, 90, 1			; falling sigmoid

    ; *************************************************
    ; example of soft synchronization of two partikkel instances
    ; *************************************************
    	instr 1

    /*score parameters*/
    igrainrate	= p4		; grain rate
    igrainsize	= p5		; grain size in ms
    igrainFreq	= p6		; fundamental frequency of source waveform
    iosc2Dev	= p7		; partikkel instance 2 grain rate deviation factor
    iMaxSync	= p8		; max soft sync amount (increasing to this value during length of note)

    /*overall envelope*/
    iattack		= 0.001
    idecay		= 0.2
    isustain	= 0.7
    irelease	= 0.2
    amp		linsegr	0, iattack, 1, idecay, isustain, 1, isustain, irelease, 0

    kgrainfreq	= igrainrate		; grains per second
    kdistribution	= 0			; periodic grain distribution
    idisttab	= -1			; (default) flat distribution used
                                            ; for grain distribution
    async		= 0			; no sync input
    kenv2amt	= 0			; no secondary enveloping
    ienv2tab	= -1			; default secondary envelope (flat)
    ienv_attack	= giSigmoRise		; default attack envelope (flat)
    ienv_decay	= giSigmoFall		; default decay envelope (flat)
    ksustain_amount	= 0.3			; time (in fraction of grain dur) at
                                            ; sustain level for each grain
    ka_d_ratio	= 0.2 			; balance between attack and decay time
    kduration	= igrainsize		; set grain duration in ms
    kamp		= 0.2*0dbfs 		; amp
    igainmasks	= -1			; (default) no gain masking
    kwavfreq	= igrainFreq		; fundamental frequency of source waveform
    ksweepshape	= 0			; shape of frequency sweep (0=no sweep)
    iwavfreqstarttab = -1			; default frequency sweep start
                                            ; (value in table = 1, which give
                                            ; no frequency modification)
    iwavfreqendtab	= -1			; default frequency sweep end
                                            ; (value in table = 1, which give
                                            ; no frequency modification)
    awavfm		= 0			; no FM input
    ifmamptab	= -1			; default FM scaling (=1)
    kfmenv		= -1			; default FM envelope (flat)
    icosine		= giCosine		; cosine ftable
    kTrainCps	= kgrainfreq		; set trainlet cps equal to grain
                                            ; rate for single-cycle trainlet in
                                            ; each grain
    knumpartials	= 3			; number of partials in trainlet
    kchroma		= 1			; balance of partials in trainlet
    ichannelmasks	= -1			; (default) no channel masking,
                                            ; all grains to output 1
    krandommask	= 0			; no random grain masking
    kwaveform1	= giSine		; source waveforms
    kwaveform2	= giSine		;
    kwaveform3	= giSine		;
    kwaveform4	= giSine		;
    iwaveamptab	= -1			; mix of 4 source waveforms and
                                            ; trainlets (set to default)
    asamplepos1	= 0			; phase offset for reading source waveform
    asamplepos2	= 0			;
    asamplepos3	= 0			;
    asamplepos4	= 0			;
    kwavekey1	= 1			; original key for source waveform
    kwavekey2	= 1			;
    kwavekey3	= 1			;
    kwavekey4	= 1			;
    imax_grains	= 100			; max grains per k period
    iopcode_id	= 1			; id of opcode, linking partikkel
                                            ; to partikkelsync

    a1  partikkel kgrainfreq, kdistribution, idisttab, async, kenv2amt, \
           ienv2tab,ienv_attack, ienv_decay, ksustain_amount, ka_d_ratio, \
           kduration, kamp, igainmasks, kwavfreq, ksweepshape, \
           iwavfreqstarttab, iwavfreqendtab, awavfm, ifmamptab, kfmenv, \
           icosine, kTrainCps, knumpartials, kchroma, ichannelmasks, \
           krandommask, kwaveform1, kwaveform2, kwaveform3, kwaveform4, \
           iwaveamptab, asamplepos1, asamplepos2, asamplepos3, asamplepos4, \
           kwavekey1, kwavekey2, kwavekey3, kwavekey4, imax_grains, iopcode_id

    async1		partikkelsync	iopcode_id   ; clock pulse output of the
                                                 ; partikkel instance above
    ksyncGravity 	line 0, p3, iMaxSync	     ; strength of synchronization
    aphase2		init 0
    asyncPolarity	limit (int(aphase2*2)*2)-1, -1, 1
    ; use the phase of partikkelsync instance 2 to find sync
    ; polarity for partikkel instance 2.
    ; If the phase of instance 2 is less than 0.5, we want to
    ; nudge it down when synchronizing,
    ; and if the phase is > 0.5 we want to nudge it upwards.
    async1		= async1*ksyncGravity*asyncPolarity  ; prepare sync signal
                                                      ; with polarity and strength

    kgrainfreq2	= igrainrate * iosc2Dev		; grains per second for second partikkel instance
    iopcode_id2	= 2
    a2 partikkel kgrainfreq2, kdistribution, idisttab, async1, kenv2amt, \
           ienv2tab, ienv_attack, ienv_decay, ksustain_amount, ka_d_ratio, \
           kduration, kamp, igainmasks, kwavfreq, ksweepshape, \
           iwavfreqstarttab, iwavfreqendtab, awavfm, ifmamptab, kfmenv, \
           icosine, kTrainCps, knumpartials, kchroma, ichannelmasks, \
           krandommask, kwaveform1, kwaveform2, kwaveform3, kwaveform4, \
           iwaveamptab, asamplepos1, asamplepos2, asamplepos3, \
           asamplepos4, kwavekey1, kwavekey2, kwavekey3, kwavekey4, \
           imax_grains, iopcode_id2

    async2, aphase2	partikkelsync	iopcode_id2
    ; clock pulse and phase
    ; output of the partikkel instance above,
    ; we will only use the phase

    outs	a1*amp, a2*amp

    endin

    </CsInstruments>
    <CsScore>

    /*score parameters
    igrainrate	= p4		; grain rate
    igrainsize	= p5		; grain size in ms
    igrainFreq	= p6		; frequency of source wave within grain
    iosc2Dev	= p7		; partikkel instance 2 grain rate deviation factor
    iMaxSync	= p8		; max soft sync amount (increasing to this value during length of note)
    */
    ;		GrRate	GrSize	GrFund	Osc2Dev	MaxSync

    i1 0 	10	2	20	880	1.3	0.3
    s
    i1 0 	10	5	20	440	0.8	0.3
    s
    i1 0 	6	55	15	660	1.8	0.45
    s
    i1 0 	6	110	10	440	0.6	0.6
    s
    i1 0 	6	220	3	660	2.6	0.45
    s
    i1 0 	6	220	3	660	2.1	0.45
    s
    i1 0 	6	440	3	660	0.8	0.22
    s

    e

    e
    </CsScore>
    </CsoundSynthesizer>

## Voir aussi

partikkel

## Crédits

Auteur : Thom Johansen
Auteur : Torgeir Strand Henriksen
Auteur : Øyvind Brandtsegg
Avril 2007

Nouveau dans la version 5.06

Précédent | Niveau supérieur | Suivant
partikkel | Sommaire | passign