rtclock
Précédent | Opcodes et opérateurs de l'orchestre | Suivant

## rtclock

rtclock — Lit l'horloge temps réel du système d'exploitation.

## Description

Lit l'horloge temps réel du système d'exploitation.

## Syntaxe

    ires rtclock

    kres rtclock

## Exécution

Lit l'horloge temps réel du système d'exploitation. Sous Windows, celle-ci ne change qu'une fois par seconde. Sous GNU/Linux, elle change chaque microseconde. Le comportement sous les autres systèmes varie.

## Exemples

Voici un exemple de l'opcode rtclock. Il utilise le fichier rtclock.csd.

Exemple 804. Exemple de l'opcode rtclock.

Voir les sections Audio en Temps Réel et Options de la Ligne de Commande pour plus d'information sur l'utilisation des options de la ligne de commande.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -n     ;;;no sound
    ;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o rtclock.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    ;after an example by Iain McCurdy

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    FLcolor	200, 200, 200, 0, 0, 0
    ;	LABEL     | WIDTH | HEIGHT | X | Y
    FLpanel	"rtclock",   500,    130,    0,  0
    ;                                  ON,OFF,TYPE,WIDTH, HEIGHT, X, Y, OPCODE, INS,START,IDUR
    gkOnOff,ihOnOff	FLbutton "On/Off", 1,  0,  22,  150,   25,    5, 5,    0,   1,   0,   3600
    gkExit,ihExit	FLbutton "exitnow",1,  0,  21,  150,   25,  345, 5,    0,  999,  0,   0.001
    FLsetColor2 255, 0, 50, ihOnOff	;reddish color

    ;VALUE DISPLAY BOXES	 WIDTH,HEIGHT,X, Y
    gidclock FLvalue "clock", 100, 25, 200, 60
    FLsetVal_i 1, ihOnOff
    FLpanel_end
    FLrun

    instr 1

    if gkOnOff !=0 kgoto CONTINUE ;sense if FLTK on/off switch is not off (in which case skip the next line)
    turnoff			      ;turn this instr. off now
    CONTINUE:
    ktime rtclock                 ;clock continues to run even
    FLprintk2 ktime, gidclock     ;after the on/off button was used to stop

    endin

    instr 999

    exitnow			      ;exit Csound as fast as possible

    endin
    </CsInstruments>
    <CsScore>

    f 0 60	;runs 60 seconds
    e
    </CsScore>
    </CsoundSynthesizer>

## Crédits

Auteur : John ffitch

Nouveau dans la version 4.10

Précédent | Niveau supérieur | Suivant
rspline | Sommaire | S