maca
Prev | Orchestra Opcodes and Operators | Next

## maca

maca — Multiply and accumulate a-rate signals only.

## Description

Multiply and accumulate a-rate signals only.

## Syntax

    ares maca asig1 , asig2 [, asig3] [, asig4] [, asig5] [...]

## Performance

asig1, asig2, ... -- a-rate input signals

maca multiplies and accumulates a-rate signals only. It is equivalent to:

ares = asig1*asig2 + asig3*asig4 + asig5*asig6 + ...

## Examples

Here is an example of the maca opcode. It uses the file maca.csd. It is written for *NIX systems, and will generate errors on Windows.

Example 483. Example of the maca opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac     ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if real audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o mac.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    instr 1	;4 band equalizer

    klow =	p4	;low gain1
    aenv1   oscil   0.2, 1, 4
    aenv1 = aenv1 + klow
    klmid =	p5	;low gain2
    aenv2   oscil   0.21, 1.1, 4
    aenv2 = aenv2 + klmid
    kmidh = p6	;high gain1
    aenv3   oscil   0.19, 1.2, 4
    aenv3 = aenv3 + kmidh
    khigh =	p7	;high gain2
    aenv4   oscil   0.18, 1.3, 4
    aenv4 = aenv4 + khigh

    ifn  =  p8	;table

    ilc1 table 0, ifn	;low freqency range
    ilc2 table 1, ifn	;low-mid
    ihc1 table 2, ifn	;mid-high
    ihc2 table 3, ifn	;high

    asig	diskin2	 "fox.wav", 1
    alow1	butterlp asig, ilc1		;lowpass 1
    almid	butterlp asig, ilc2	      	;lowpass 2
    amidh 	butterhp asig, ihc1	       	;highpass 1
    ahigh	butterhp asig, ihc2		;highpass 2
    aout	maca	 aenv1, alow1, aenv2, almid, aenv3, amidh, aenv4, ahigh
            outs	 aout, aout

    endin
    </CsInstruments>
    <CsScore>
    f1 0  4 -2 150 300 600  5000
    f2 0  4 -2 75  500 1000 10000
    f3 0  4 -2 200 700 1500 3000
    f4 0  4096 10 1

    ;          low lowmid midhigh high table
    i 1 0  2.8  2    1      1      1     1
    i 1 3  2.8  2    3      1      1     2
    i 1 6  2.8  2    1      2      3     3
    e
    </CsScore>
    </CsoundSynthesizer>

## See Also

mac

## Credits

Author: John ffitch
University of Bath, Codemist, Ltd.
Bath, UK
May 1999

New in Csound version 3.54

Prev | Up | Next
mac | Home | madsr