vdelayx
Prev | Orchestra Opcodes and Operators | Next

## vdelayx

vdelayx — A variable delay opcode with high quality interpolation.

## Description

A variable delay opcode with high quality interpolation.

## Syntax

    aout vdelayx ain, adl, imd, iws [, ist]

## Initialization

imd -- max. delay time (seconds)

iws -- interpolation window size (see below)

ist (optional) -- skip initialization if not zero

## Performance

aout -- output audio signal

ain -- input audio signal

adl -- delay time in seconds

This opcode uses high quality (and slow) interpolation, that is much more accurate than the currently available linear and cubic interpolation. The iws parameter sets the number of input samples used for calculating one output sample (allowed values are any integer multiply of 4 in the range 4 - 1024); higher values mean better quality and slower speed.

| Notes
Delay time is measured in seconds (unlike in vdelay and vdelay3), and must be a-rate. The minimum allowed delay is iws/2 samples. Using the same variables as input and output is allowed in these opcodes. In vdelayxw*, changing the delay time has some effects on output volume: a = 1 / (1 + dt) where a is the output gain, and dt is the change of delay time per seconds. These opcodes are best used in the double-precision version of Csound.

## Examples

Here is an example of the use of the vdelayx opcode. It uses the file vdelayx.csd.

Example 1018. Example of the vdelayx opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac  ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o vdelayx.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    instr 1

    ims  =	.5				;maximum delay time in seconds
    iws  =	1024				;window size
    adl  =	.5				;delay time
    asig diskin2 "fox.wav", 1, 0, 1		;loop fox.wav
    a2   poscil .2, .2, 1			;make an LFO
    adl  = a2 + ims/2      			;offset the LFO so that it is positive
    aout vdelayx asig, adl, ims, iws	;use the LFO to control delay time
         outs aout, aout

    endin
    </CsInstruments>
    <CsScore>
    f1 0 8192 10 1

    i 1 0 10

    e
    </CsScore>
    </CsoundSynthesizer>

## See Also

vdelayxq, vdelayxs, vdelayxw, vdelayxwq, vdelayxws

Prev | Up | Next
vdelay3 | Home | vdelayxq