GEN27
Prev | Score Statements and GEN Routines | Next

## GEN27

GEN27 — Construct functions from segments of straight lines in breakpoint fashion.

## Description

Construct functions from segments of straight lines in breakpoint fashion.

## Syntax

    f # time size 27 x1  y1 x2 y2 x3 ...

## Initialization

size -- number of points in the table. Must be a power of 2 or power-of-2 plus 1 (see f statement).

x1, x2, x3, etc. -- locations in table at which to attain the following y value. Must be in increasing order. If the last value is less than size, then the rest will be set to zero. Should not be negative but can be zero.

y1, y2, y3,, etc. -- Breakpoint values attained at the location specified by the preceding x value.

| Note
If p4 is positive, functions are post-normalized (rescaled to a maximum absolute value of 1 after generation). A negative p4 will cause rescaling to be skipped.

## Examples

Here is an example of the GEN27 generator. It uses the file gen27.csd.

Example 1147. Example of the GEN27 generator.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac  ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o gen27.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    gisin ftgen 1, 0, 32768, 10, 1
    gienv ftgen 2, 0, 1025, 27, 0, 0,200, 1, 400, -1, 513, 0

    instr 1

    kcps init 3/p3			;play 3x over duration of note
    kndx phasor kcps
    ixmode = 1			;normalize to 0-1
    kval table kndx, gienv, ixmode
    kval = kval*100			;scale 0-100
    asig poscil 1, 220+kval, 1	;add to 220 Hz
         outs asig, asig

    endin
    </CsInstruments>
    <CsScore>

    i 1 0 4

    e
    </CsScore>
    </CsoundSynthesizer>

This is the diagram of the waveform of the GEN27 routine, as used in the example:

f 2 0 1025 27 0 0 200 1 400 -1 513 0 - a function which begins at 0, rises to 1 at the 200th table location, falls to -1, by the 400th location, and returns to 0 by the end of the table. The interpolation is linear

## See Also

f statement, GEN25

## Credits

Author: John ffitch
University of Bath/Codemist Ltd.
Bath, UK

New in Csound version 3.49

Prev | Up | Next
GEN25 | Home | GEN28