cossegr
Prev | Orchestra Opcodes and Operators | Next

## cossegr

cossegr — Trace a series of line segments between specified points with cosine interpolation, including a release segment.

## Description

Trace a series of line segments between specified points with cosine interpolation, including a release segment.

## Syntax

    ares cossegr ia, idur1, ib [, idur2] [, ic] [...], irel, iz

    kres cossegr ia, idur1, ib [, idur2] [, ic] [...], irel, iz

## Initialization

ia -- starting value.

ib, ic, etc. -- value after dur1 seconds, etc.

idur1 -- duration in seconds of first segment. A zero or negative value will cause all initialization to be skipped.

idur2, idur3, etc. -- duration in seconds of subsequent segments. A zero or negative value will terminate the initialization process with the preceding point, permitting the last-defined line or curve to be continued indefinitely in performance. The default is zero.

irel, iz -- duration in seconds and final value of a note releasing segment.

## Performance

These units generate control or audio signals whose values can pass through 2 or more specified points. The sum of dur values may or may not equal the instrument's performance time: a shorter performance will truncate the specified pattern, while a longer one will cause the last-defined segment to continue on in the same direction.

cossegr is amongst the Csound “r” units that contain a note-off sensor and release time extender. When each senses an event termination or MIDI noteoff, it immediately extends the performance time of the current instrument by irel seconds, and sets out to reach the value iz by the end of that period (no matter which segment the unit is in). “r” units can also be modified by MIDI noteoff velocities. For two or more extenders in an instrument, extension is by the greatest period.

You can use other pre-made envelopes which start a release segment upon receiving a note off message, like linenr and expsegr, or you can construct more complex envelopes using xtratim and release. Note that you don't need to use xtratim if you are using cossegr, since the time is extended automatically.

## Examples

Here is an example of the cossegr opcode. It uses the file cossegr.csd.

Example 148. Example of the cossegr opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac  -+rtmidi=virtual -M0   ;;;realtime audio out and realtime midi in
    ;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o linsegr.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    instr 1

    icps	cpsmidi
    iamp	ampmidi	.3

    kenv	cossegr	1, .05, 0.5, 1, 0
    asig	pluck	kenv, icps, 200, 1, 1
    	outs	asig, asig

    endin
    </CsInstruments>
    <CsScore>
    f 1 0 4096 10 1	;sine wave

    f0 30	;runs 30 seconds
    e
    </CsScore>
    </CsoundSynthesizer>

## See Also

linenr, linsegr, expsegr, envlpxr, mxadsr, madsr expon, expseg, expsega line, linseg, xtratim, transegr

## Credits

Author: John ffitch

August 2012.

New in Csound 5.18

Prev | Up | Next
cossegb | Home | cosh