hdf5write
Prev | Orchestra Opcodes and Operators | Next

## hdf5write

hdf5write — Write signals and arrays to an hdf5 file.

## Description

hdf5write writes N signals and arrays to a specified hdf5 file.

## Syntax

    hdf5write ifilename, xout1[, xout2, xout3, ..., xoutN]

## Initialization

ifilename -- the hdf5 file's name (in double-quotes). If the file does not exist it will be created.

## Performance

xout1,... xoutN -- signals or arrays to be written to the hdf5 file. This opcode accepts i-rate, k-rate, a-rate signals or i-rate, k-rate, a-rate arrays of any dimension. These signals or arrays are written to a dataset within the hdf5 file using the same variable name as in Csound. For example, if the Csound variable is called 'ksignal', then the name of the hdf5 dataset is 'ksignal'. Any number and multiple types of datasets may be written at a time.

## Examples

Here is a simple example of the hdf5write opcode. It uses the file hdf5write.csd.

Example 383. Example of the hdf5write opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    -odac
    </CsOptions>
    <CsInstruments>
    nchnls = 2
    0dbfs = 1
    ksmps = 8
    sr = 44100

    instr hdf5write

        aArray[] init 2,2 ; Initialise a 2 X 2 a-rate array

        aArray[0][0] vco2 0.2, 100 ; Fill array with vco2 signals
        aArray[0][1] vco2 0.4, 200
        aArray[1][0] vco2 0.8, 300
        aArray[1][1] vco2 1, 400

        aVar vco2 0.2, 100 ; Initialise an a-rate variable with a vco2 signal

        kVar phasor 1 ; Initalise a k-rate variable with a phasor signal

        hdf5write "example.h5", aArray, aVar, kVar ; Write variables to an hdf5 file

    endin

    </CsInstruments>
    <CsScore>

    i "hdf5write" 0 1

    </CsScore>
    </CsoundSynthesizer>

## See Also

hdf5read

## Credits

Author: Edward Costello;
NUIM, 2014

Prev | Up | Next
hdf5read | Home | hilbert