tabrec
Prev | Orchestra Opcodes and Operators | Next

## tabrec

tabrec — Recording of control signals.

## Description

Records control-rate signals on trigger-temporization basis.

## Syntax

    tabrec   ktrig_start, ktrig_stop, knumtics, kfn, kin1 [,kin2,...,kinN]

## Performance

ktrig_start -- start recording when non-zero.

ktrig_stop -- stop recording when knumtics trigger impulses are received by this input argument.

knumtics -- stop recording or reset playing pointer to zero when the number of tics defined by this argument is reached.

kfn -- table where k-rate signals are recorded.

kin1,...,kinN -- input signals to record.

The tabrec and tabplay opcodes allow to record/playback control signals on trigger-temporization basis.

tabrec opcode records a group of k-rate signals by storing them into kfn table. Each time ktrig_start is triggered, tabrec resets the table pointer to zero and begins to record. Recording phase stops after knumtics trigger impulses have been received by ktrig_stop argument.

These opcodes can be used like a sort of ``middle-term'' memory that ``remembers'' generated signals. Such memory can be used to supply generative music with a coherent iterative compositional structure.

## See Also

tabplay

## Credits

Written by Gabriel Maldonado.

Prev | Up | Next
tabplay | Home | tabsum