lowpass2
Prev | Orchestra Opcodes and Operators | Next

## lowpass2

lowpass2 — A resonant lowpass filter.

## Description

Implementation of a resonant second-order lowpass filter.

## Syntax

    ares lowpass2 asig, kcf, kq [, iskip]

## Initialization

iskip -- initial disposition of internal data space. A zero value will clear the space; a non-zero value will allow previous information to remain. The default value is 0.

## Performance

asig -- input signal to be filtered

kcf -- cutoff or resonant frequency of the filter, measured in Hz

kq -- Q of the filter, defined, for bandpass filters, as bandwidth/cutoff. kq should be between 1 and 500

lowpass2 is a second order IIR lowpass filter, with k-rate controls for cutoff frequency (kcf) and Q (kq). As kq is increased, a resonant peak forms around the cutoff frequency, transforming the lowpass filter response into a response that is similar to a bandpass filter, but with more low frequency energy. This corresponds to an increase in the magnitude and "sharpness" of the resonant peak. For high values of kq, a scaling function such as balance may be required. In practice, this allows for the simulation of the voltage-controlled filters of analog synthesizers, or for the creation of a pitch of constant amplitude while filtering white noise.

## Examples

Here is an example of the lowpass2 opcode. It uses the file lowpass2.csd.

Example 465. Example of the lowpass2 opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    ; Audio out   Audio in    No messages
    -odac           -iadc     -d     ;;;RT audio I/O
    ; For Non-realtime ouput leave only the line below:
    ; -o lowpass2.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    /* Written by Sean Costello */
    ; Orchestra file for resonant filter sweep of a sawtooth-like waveform.
      sr = 44100
      kr = 2205
      ksmps = 20
      nchnls = 1

              instr 1

      idur    =          p3
      ifreq   =          p4
      iamp    =          p5 * .5
      iharms  =          (sr*.4) / ifreq

    ; Sawtooth-like waveform
      asig    gbuzz 1, ifreq, iharms, 1, .9, 1

    ; Envelope to control filter cutoff
      kfreq   linseg 1, idur * 0.5, 5000, idur * 0.5, 1

      afilt   lowpass2 asig,kfreq, 30

    ; Simple amplitude envelope
      kenv    linseg 0, .1, iamp, idur -.2, iamp, .1, 0
              out afilt * kenv

              endin

    </CsInstruments>
    <CsScore>

    /* Written by Sean Costello */
    f1 0 8192 9 1 1 .25

    i1 0 5 100 1000
    i1 5 5 200 1000
    e

    </CsScore>
    </CsoundSynthesizer>

## Credits

Author: Sean Costello
Seattle, Washington
August 1999

New in Csound version 4.0

Prev | Up | Next
loscilx | Home | lowres