outkpc
Prev | Orchestra Opcodes and Operators | Next

## outkpc

outkpc — Sends MIDI program change messages at k-rate.

## Description

Sends MIDI program change messages at k-rate.

## Syntax

    outkpc kchn, kprog, kmin, kmax

## Performance

kchn -- MIDI channel number (1-16)

kprog -- program change number in floating point

kmin -- minimum floating point value (converted in MIDI integer value 0)

kmax -- maximum floating point value (converted in MIDI integer value 127 (7 bit))

outkpc (k-rate program change output) sends program change messages. It works only with MIDI instruments which recognize them. These opcodes can drive a different value of a parameter for each note currently active.

It can scale the k-value floating-point argument according to the kmin and kmax values. For example: set kmin = 1.0 and kmax = 2.0. When the kvalue argument receives a 2.0 value, the opcode will send a 127 value to the MIDI OUT device. When the kvalue argument receives a 1.0 value, it will send a 0 value. k-rate opcodes send a message each time the MIDI converted value of argument kvalue changes.

## Examples

Here is an example of the outkpc opcode. It uses the file outkpc.csd.

Example 607. Example of the outkpc opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

This example generates a program change and a note on Csound's MIDI output port whenever a note is received on channel 1. Be sure to have something connected to Csound's MIDI out port to hear the result.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    ; Audio out   Audio in    No messages
    -odac           -iadc     -d         -M0  -Q1 ;;;RT audio I/O with MIDI in
    </CsOptions>
    <CsInstruments>

    sr = 44100
    kr = 4410
    ksmps = 10
    nchnls = 2

    ; Example by Giorgio Zucco 2007

    kprogram init 0

    instr 1 ;Triggered by MIDI notes on channel 1

      ifund   notnum
      ivel 	veloc
      idur = 1

    ; Sends a MIDI program change message according to
    ; the triggering note's velocity
    outkpc     1 ,ivel ,0 ,127

    noteondur  1 ,ifund ,ivel ,idur

    endin

    </CsInstruments>
    <CsScore>
    ; Dummy ftable
    f 0 60
    </CsScore>
    </CsoundSynthesizer>

Here is another example of the outkpc opcode. It uses the file outkpc_flkt.csd.

Example 608. Example of the outkpc opcode using FLTK.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    ; Audio out   Audio in    No messages
    -odac           -iadc     -d         -M0  -Q1;;;RT audio I/O with MIDI in
    </CsOptions>
    <CsInstruments>

    sr = 44100
    kr = 4410
    ksmps = 10
    nchnls = 2

    ; Example by Giorgio Zucco 2007

    FLpanel "outkpc",200,100,90,90;start of container
    gkpg, gihandle FLcount "Midi-Program change",0,127,1,5,1,152,40,16,23,-1
    FLpanelEnd

    FLrun

    instr 1

    ktrig changed gkpg
    outkpc     ktrig,gkpg,0,127

    endin

    </CsInstruments>
    <CsScore>
    ; Run instrument 1 for 60 seconds
    i 1 0  60
    </CsScore>
    </CsoundSynthesizer>

## See Also

outiat, outic14, outic, outipat, outipb, outipc, outkat, outkc14, outkc, outkpat, outkpb

## Credits

Author: Gabriel Maldonado
Italy

New in Csound version 3.47

Thanks goes to Rasmus Ekman for pointing out the correct MIDI channel and controller number ranges.

Prev | Up | Next
outkpb | Home | outleta