alwayson
Précédent | Opcodes et opérateurs de l'orchestre | Suivant

## alwayson

alwayson — Active les instruments indiqués dans l'en-tête de l'orchestre sans le recours à une instruction i.

## Description

Active les instruments indiqués dans l'en-tête de l'orchestre sans le recours à une instruction i. Les instruments doivent être activés dans le même ordre que celui de leur définition.

L'opcode alwayson est conçu pour simplifier la définition d'orchestres réutilisables avec traitement du signal ou enchainement d'effets et réseaux.

## Syntaxe

     alwayson Tinstrument [p4, ..., pn]

## Initialisation

Tinstrument -- Nom sous forme de chaîne de caractères de la définition d'instrument à activer.

[p4, ..., pn] -- p-champs optionnels à passer à l'instrument, dans le même ordre et avec les mêmes types que si c'était une instruction i.

Lors de l'activation de l'instrument, p1 est son numéro, p2 vaut 0 et p3 vaut -1. Les p-champs à partir de p4 peuvent être envoyés à l'instrument de manière optionnelle.

## Exemples

Voici un exemple de l'opcode alwayson. Il utilise le fichier alwayson.csd.

Exemple 50. Exemple de l'opcode alwayson.

    <CsoundSynthesizer>
    <CsOptions>

    ; Select audio/midi flags here according to platform
    -odac     ;;;RT audio out
    ;-iadc    ;;;uncomment -iadc if RT audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ;-Wfo alwayson.wav
    </CsOptions>
    <CsInstruments>

    ; Initialize the global variables.

    sr     = 44100
    ksmps 	= 32
    nchnls 	= 2

    ; Connect up instruments and effects to create the signal flow graph.

    connect "SimpleSine",   	"leftout",     "Reverberator",     	"leftin"
    connect "SimpleSine",   	"rightout",    "Reverberator",     	"rightin"

    connect "Moogy",        	"leftout",     "Reverberator",     	"leftin"
    connect "Moogy",        	"rightout",    "Reverberator",     	"rightin"

    connect "Reverberator", 	"leftout",     "Compressor",       	"leftin"
    connect "Reverberator", 	"rightout",    "Compressor",       	"rightin"

    connect "Compressor",   	"leftout",     "Soundfile",       	"leftin"
    connect "Compressor",   	"rightout",    "Soundfile",       	"rightin"

    ; Turn on the "effect" units in the signal flow graph.

    alwayson "Reverberator", 0.91, 12000
    alwayson "Compressor"
    alwayson "Soundfile"

    ; Define instruments and effects in order of signal flow.

    			    instr SimpleSine
                    ;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
    			    ; Default values:   p1  p2  p3  p4  p5  p6  p7  p8  p9  p10
    			    pset			    0,  0,  10, 0,  0,  0,  0.5
    iattack			=			        0.015
    idecay			=			        0.07
    isustain		=			        p3
    irelease		=			        0.3
    p3			    =			        iattack + idecay + isustain + irelease
    adamping		linsegr			    0.0, iattack, 1.0, idecay + isustain, 1.0, irelease, 0.0
    iHz 			= 			        cpsmidinn(p4)
                    ; Rescale MIDI velocity range to a musically usable range of dB.
    iamplitude 		= 			        ampdb(p5 / 127 * 15.0 + 60.0)
    			    ; Use ftgenonce instead of ftgen, ftgentmp, or f statement.
    icosine			ftgenonce 		    0, 0, 65537, 11, 1
    aoscili			oscili 			    iamplitude, iHz, icosine
    aadsr 			madsr 			    iattack, idecay, 0.6, irelease
    asignal 		= 			        aoscili * aadsr
    aleft, aright	pan2			    asignal, p7
    			    ; Stereo audio output to be routed in the orchestra header.
    			    outleta 		    "leftout", aleft
    			    outleta 		    "rightout", aright
    			    endin

    			    instr Moogy
                    ;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
    			    ; Default values:   p1  p2  p3  p4  p5  p6  p7  p8  p9  p10
    			    pset			    0,  0,  10, 0,  0,  0,  0.5
    iattack			=			        0.003
    isustain		=			        p3
    irelease		=			        0.05
    p3			    =			        iattack + isustain + irelease
    adamping		linsegr			    0.0, iattack, 1.0, isustain, 1.0, irelease, 0.0
    iHz 			= 			        cpsmidinn(p4)
                    ; Rescale MIDI velocity range to a musically usable range of dB.
    iamplitude 		= 			        ampdb(p5 / 127 * 20.0 + 60.0)
    			    print 			    iHz, iamplitude
    			    ; Use ftgenonce instead of ftgen, ftgentmp, or f statement.
    isine 			ftgenonce 		    0, 0, 65537, 10, 1
    asignal 		vco 			    iamplitude, iHz, 1, 0.5, isine
    kfco 			line 			    2000, p3, 200
    krez 			= 			        0.8
    asignal 		moogvcf 		    asignal, kfco, krez, 100000
    asignal			=			        asignal * adamping
    aleft, aright	pan2			    asignal, p7
    			    ; Stereo audio output to be routed in the orchestra header.
    			    outleta 		    "leftout", aleft
    			    outleta 		    "rightout", aright
    			    endin
    			    instr Reverberator
                    ;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
    			    ; Stereo input.
    aleftin 		inleta 			    "leftin"
    arightin 		inleta 			    "rightin"
    idelay 			= 			        p4
    icutoff 		= 			        p5
    aleft, aright 	reverbsc 	        aleftin, arightin, idelay, icutoff
    			    ; Stereo output.
    			    outleta 	        "leftout", aleft
    			    outleta 	        "rightout", aright
    			    endin

    			    instr Compressor
                    ;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
    			    ; Stereo input.
    aleftin 		inleta 		        "leftin"
    arightin 		inleta 		        "rightin"
    kthreshold 		= 		            25000
    icomp1 			= 		            0.5
    icomp2 			= 		            0.763
    irtime 			= 		            0.1
    iftime 			= 		            0.1
    aleftout 		dam 		        aleftin, kthreshold, icomp1, icomp2, irtime, iftime
    arightout 		dam 		        arightin, kthreshold, icomp1, icomp2, irtime, iftime
    			    ; Stereo output.
    			    outleta 	        "leftout", aleftout
    			    outleta 	        "rightout", arightout
    			    endin

    			    instr Soundfile
                    ;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
    			    ; Stereo input.
    aleftin 		inleta 		        "leftin"
    arightin 		inleta 		        "rightin"
    			    outs 		        aleftin, arightin
    			    endin

    </CsInstruments>
    <CsScore>

    ; It is not necessary to activate "effects" or create f-tables in the score!
    ; Overlapping notes create new instances of instruments with proper connections.

    i "SimpleSine" 1 5 60 85
    i "SimpleSine" 2 5 64 80
    i "Moogy" 3 5 67 75
    i "Moogy" 4 5 71 70
    ; 1 extra second after the performance
    e 1

    </CsScore>
    </CsoundSynthesizer>

## Crédits

Par Michael Gogins, 2009

Précédent | Niveau supérieur | Suivant
alpass | Sommaire | ampdb