vstnote
Précédent | Opcodes et opérateurs de l'orchestre | Suivant

## vstnote

vstnote — Envoie une note MIDI de durée définie à un greffon VST.

## Syntaxe

    vstnote instance, kchan, knote, kveloc, kdur

## Description

vstnote envoie une note MIDI de durée définie à un greffon VST.

## Initialisation

instance - le numéro qui identifie le greffon, généré par vstinit.

## Exécution

kchan - Le canal MIDI de transmission. Noter que les canaux MIDI sont numérotés à partir de 0.

knote - Le numéro de la note MIDI à envoyer.

kveloc - La vélocité de la note MIDI.

kdur - La durée de la note MIDI en secondes.

Note : il faut s'assurer que l'instrument contenant vstnote ne se termine pas avant que la durée de la note ne soit écoulée, sinon on aura une note tenue indéfiniment.

## Exemples

Voici un exemple de l'opcode vstnote. Il utilise le fichier vst4cs.csd.

Exemple 1062. Exemple de l'opcode vstnote.

Voir les sections Audio en Temps Réel et Options de la Ligne de Commande pour plus d'information sur l'utilisation des options de la ligne de commande.

    <CsoundSynthesizer>
    <CsOptions>
    ; Credits: Adapted by Michael Gogins
    ; from code by David Horowitz and Lian Cheung.
    ; The "--displays" option is required in order for
    ; the Pianoteq GUI to dispatch events and display properly.
    -m3 --displays -odac
    </CsOptions>
    <CsInstruments>
    sr     = 44100
    ksmps  = 20
    nchnls = 2
                    ; Load the Pianoteq into memory.
    gipianoteq      vstinit         "C:\\Program Files\\Steinberg\\VstPlugins\\Pianoteq 3.0 Trial\\Pianoteq30 Trial.dll", 1

                    ; Print information about the Pianoteq, such as parameter names and numbers.
                    vstinfo         gipianoteq

                    ; Open the Pianoteq's GUI.
                    vstedit         gipianoteq

                    ; Send notes from the score to the Pianoteq.
                    instr 1
                    ; MIDI channels are numbered starting at 0.
                    ; p3 always contains the duration of the note.
                    ; p4 contains the MIDI key number (pitch),
                    ; p5 contains the MIDI velocity number (loudness),
    imidichannel    init            0
                    vstnote         gipianoteq, imidichannel, p4, p5, p3
                    endin

                    ; Send parameter changes to the Pianoteq.
                    instr 2
                    ; p4 is the parameter number.
                    ; p5 is the parameter value.
                    vstparamset     gipianoteq, p4, p5
                    endin

                    ; Send audio from the Pianoteq to the output.
                    instr 3
    ablankinput     init            0
    aleft, aright   vstaudio        gipianoteq, ablankinput, ablankinput
                    outs            aleft, aright
                    endin

    </CsInstruments>
    <CsScore>
    ; Turn on the instrument that receives audio from the Pianoteq indefinitely.
    i 3 0 -1
    ; Send parameter changes to Pianoteq before sending any notes.
    ; NOTE: All parameters must be between 0.0 and 1.0.
    ; Length of piano strings:
    i 2 0 1 33 0.5
    ; Hammer noise:
    i 2 0 1 25 0.1
    ; Send a C major 7th arpeggio to the Pianoteq.
    i 1 1 10 60 76
    i 1 2 10 64 73
    i 1 3 10 67 70
    i 1 4 10 71 67
    ; End the performance, leaving some time
    ; for the Pianoteq to finish sending out its audio,
    ; or for the user to play with the Pianoteq virtual keyboard.
    e 20
    </CsScore>
    </CsoundSynthesizer>

## Crédits

Par Andrés Cabrera et Michael Gogins

Utilise du code de VSTHost par Hermann Seib et de l'objet vst~ par Thomas Grill.

VST est une marque déposée de Steinberg Media Technologies GmbH. Technologie de greffon VST par Steinberg.

Précédent | Niveau supérieur | Suivant
vstmidiout | Sommaire | vstparamset,vstparamget