Moravian Instruments CCD Driver
===============================

This package provides Moravian Instruments CCD INDI driver for MI CCD cameras.

Requirements
============

+ INDI >= v1.2.0 (http://www.indilib.org/)

	You need to install both indi and indi-devel to build this package.

+ cfitsio

	cfitsio-devel is required to compile support for FITS.

+ libusb-1

	libusb-1 is required.

Installation
============

	See INSTALL

How to Use
==========

	You can use the MI INDI Driver in any INDI-compatible client such as KStars or Xephem.

	To run the driver from the command line:

	USB variant:

	$ indiserver indi_mi_ccd_usb

	ETH variant:

	$ indiserver indi_mi_ccd_eth

	You can then connect to the driver from any client, the default port is 7624.
	If you're using KStars, the driver will be automatically listed in KStars' Device Manager,
	no further configuration is necessary.
