Meade DSI Pro I/II
=================================
This package provides the INDI driver for the Meade DSI Pro I/II.

Requirements
============
* INDI
* CFITSIO
* libusb


Installation
============
See INSTALL


How to Use
==========
Once installed, the Meade DSI Pro I/II INDI driver can be used by an INDI client such as
KStars (Ekos) or OpenPHD. It can also be used manually by invoking it via the 
indi_server:
$ indi_server indi_dsi_ccd


Important!!!
============
The Meade DSI uses a Cypress EZUSB FX2 controller which requires firmware to be
loaded before the device is usable (as a DSI).
