- NAT Networks
- Host-only Networks

Active | Name
--- | ---
asdf | asdf

interface |

- Adapter
- DHCP Server

IPv4 Address: |
IPv4 Network Mask: |
IPv6 Address: |
IPv6 Network Mask Length: |

Enable Server
Server Address: |
Server Mask: |
Lower Address Bound: |
Upper Address Bound: |

Enable Network
Network Name: |
Network CIDR: |
Network Options: | Supports DHCP
| Supports IPv6
| Advertise Default IPv6 Route