#### Previous topic

scipy.signal.iirdesign

#### Next topic

scipy.signal.kaiser_atten

# scipy.signal.iirfilter

`scipy.signal.``iirfilter`(N, Wn, rp=None, rs=None, btype='band', analog=False, ftype='butter', output='ba')

  IIR digital and analog filter design given order and critical points.

  Design an Nth order digital or analog filter and return the filter coefficients.

  Parameters: | N : int The order of the filter. Wn : array_like A scalar or length-2 sequence giving the critical frequencies. For digital filters, Wn is normalized from 0 to 1, where 1 is the Nyquist frequency, pi radians/sample. (Wn is thus in half-cycles / sample.) For analog filters, Wn is an angular frequency (e.g. rad/s). rp : float, optional For Chebyshev and elliptic filters, provides the maximum ripple in the passband. (dB) rs : float, optional For Chebyshev and elliptic filters, provides the minimum attenuation in the stop band. (dB) btype : {‘bandpass’, ‘lowpass’, ‘highpass’, ‘bandstop’}, optional The type of filter. Default is ‘bandpass’. analog : bool, optional When True, return an analog filter, otherwise a digital filter is returned. ftype : str, optional The type of IIR filter to design: Butterworth : ‘butter’ Chebyshev I : ‘cheby1’ Chebyshev II : ‘cheby2’ Cauer/elliptic: ‘ellip’ Bessel/Thomson: ‘bessel’ output : {‘ba’, ‘zpk’, ‘sos’}, optional Type of output: numerator/denominator (‘ba’), pole-zero (‘zpk’), or second-order sections (‘sos’). Default is ‘ba’.
  Returns: | b, a : ndarray, ndarray Numerator (b) and denominator (a) polynomials of the IIR filter. Only returned if `output='ba'`. z, p, k : ndarray, ndarray, float Zeros, poles, and system gain of the IIR filter transfer function. Only returned if `output='zpk'`. sos : ndarray Second-order sections representation of the IIR filter. Only returned if `output=='sos'`.

  See also

  `butter`
    Filter design using order and critical points

  `cheby1`, `cheby2`, `ellip`, `bessel`

  `buttord`
    Find order and critical points from passband and stopband spec

  `cheb1ord`, `cheb2ord`, `ellipord`

  `iirdesign`
    General filter design using passband and stopband spec

  Notes

  The `'sos'` output parameter was added in 0.16.0.

  Examples

  Generate a 17th-order Chebyshev II bandpass filter and plot the frequency response:

      >>> from scipy import signal
      >>> import matplotlib.pyplot as plt

      >>> b, a = signal.iirfilter(17, [50, 200], rs=60, btype='band',
      ...                         analog=True, ftype='cheby2')
      >>> w, h = signal.freqs(b, a, 1000)
      >>> fig = plt.figure()
      >>> ax = fig.add_subplot(111)
      >>> ax.semilogx(w, 20 * np.log10(abs(h)))
      >>> ax.set_title('Chebyshev Type II bandpass frequency response')
      >>> ax.set_xlabel('Frequency [radians / second]')
      >>> ax.set_ylabel('Amplitude [dB]')
      >>> ax.axis((10, 1000, -100, 10))
      >>> ax.grid(which='both', axis='both')
      >>> plt.show()

  (Source code)