#### Previous topic

scipy.signal.csd

#### Next topic

scipy.signal.spectrogram

# scipy.signal.coherence

`scipy.signal.``coherence`(x, y, fs=1.0, window='hanning', nperseg=256, noverlap=None, nfft=None, detrend='constant', axis=-1)

  Estimate the magnitude squared coherence estimate, Cxy, of discrete-time signals X and Y using Welch’s method.

  Cxy = abs(Pxy)**2/(Pxx*Pyy), where Pxx and Pyy are power spectral density estimates of X and Y, and Pxy is the cross spectral density estimate of X and Y.

  Parameters: | x : array_like Time series of measurement values y : array_like Time series of measurement values fs : float, optional Sampling frequency of the x and y time series. Defaults to 1.0. window : str or tuple or array_like, optional Desired window to use. See `get_window` for a list of windows and required parameters. If window is array_like it will be used directly as the window and its length will be used for nperseg. Defaults to ‘hanning’. nperseg : int, optional Length of each segment. Defaults to 256. noverlap: int, optional Number of points to overlap between segments. If None, `noverlap = nperseg // 2`. Defaults to None. nfft : int, optional Length of the FFT used, if a zero padded FFT is desired. If None, the FFT length is nperseg. Defaults to None. detrend : str or function or False, optional Specifies how to detrend each segment. If `detrend` is a string, it is passed as the `type` argument to `detrend`. If it is a function, it takes a segment and returns a detrended segment. If `detrend` is False, no detrending is done. Defaults to ‘constant’. axis : int, optional Axis along which the coherence is computed for both inputs; the default is over the last axis (i.e. `axis=-1`).
  Returns: | f : ndarray Array of sample frequencies. Cxy : ndarray Magnitude squared coherence of x and y.

  See also

  `periodogram`
    Simple, optionally modified periodogram
  `lombscargle`
    Lomb-Scargle periodogram for unevenly sampled data
  `welch`
    Power spectral density by Welch’s method.
  `csd`
    Cross spectral density by Welch’s method.

  Notes

  An appropriate amount of overlap will depend on the choice of window and on your requirements. For the default ‘hanning’ window an overlap of 50% is a reasonable trade off between accurately estimating the signal power, while not over counting any of the data. Narrower windows may require a larger overlap.

  New in version 0.16.0.

  References

  [R166] | P. Welch, “The use of the fast Fourier transform for the estimation of power spectra: A method based on time averaging over short, modified periodograms”, IEEE Trans. Audio Electroacoust. vol. 15, pp. 70-73, 1967.

  [R167] | Stoica, Petre, and Randolph Moses, “Spectral Analysis of Signals” Prentice Hall, 2005

  Examples

      >>> from scipy import signal
      >>> import matplotlib.pyplot as plt

  Generate two test signals with some common features.

      >>> fs = 10e3
      >>> N = 1e5
      >>> amp = 20
      >>> freq = 1234.0
      >>> noise_power = 0.001 * fs / 2
      >>> time = np.arange(N) / fs
      >>> b, a = signal.butter(2, 0.25, 'low')
      >>> x = np.random.normal(scale=np.sqrt(noise_power), size=time.shape)
      >>> y = signal.lfilter(b, a, x)
      >>> x += amp*np.sin(2*np.pi*freq*time)
      >>> y += np.random.normal(scale=0.1*np.sqrt(noise_power), size=time.shape)

  Compute and plot the coherence.

      >>> f, Cxy = signal.coherence(x, y, fs, nperseg=1024)
      >>> plt.semilogy(f, Cxy)
      >>> plt.xlabel('frequency [Hz]')
      >>> plt.ylabel('Coherence')
      >>> plt.show()

  (Source code)