#### Previous topic

scipy.signal.gausspulse

#### Next topic

scipy.signal.sawtooth

# scipy.signal.max_len_seq

`scipy.signal.``max_len_seq`(nbits, state=None, length=None, taps=None)

  Maximum Length Sequence (MLS) generator

  Parameters: | nbits : int Number of bits to use. Length of the resulting sequence will be `(2**nbits) - 1`. Note that generating long sequences (e.g., greater than `nbits == 16`) can take a long time. state : array_like, optional If array, must be of length `nbits`, and will be cast to binary (bool) representation. If None, a seed of ones will be used, producing a repeatable representation. If `state` is all zeros, an error is raised as this is invalid. Default: None. length : int | None, optional Number of samples to compute. If None, the entire length `(2**nbits) - 1` is computed. taps : array_like, optional Polynomial taps to use (e.g., `[7, 6, 1]` for an 8-bit sequence). If None, taps will be automatically selected (for up to `nbits == 32`).
  Returns: | seq : array Resulting MLS sequence of 0’s and 1’s. state : array The final state of the shift register.

  Notes

  The algorithm for MLS generation is generically described in:

  > http://en.wikipedia.org/wiki/Maximum_length_sequence

  The default values for taps are specifically taken from the first option listed for each value of `nbits` in:

  > http://www.newwaveinstruments.com/resources/articles/
  >   m_sequence_linear_feedback_shift_register_lfsr.htm

  New in version 0.15.0.