#### Previous topic

scipy.signal.ricker

#### Next topic

scipy.signal.find_peaks_cwt

# scipy.signal.cwt

`scipy.signal.``cwt`(data, wavelet, widths)

  Continuous wavelet transform.

  Performs a continuous wavelet transform on data, using the wavelet function. A CWT performs a convolution with data using the wavelet function, which is characterized by a width parameter and length parameter.

  Parameters: | data : (N,) ndarray data on which to perform the transform. wavelet : function Wavelet function, which should take 2 arguments. The first argument is the number of points that the returned vector will have (len(wavelet(width,length)) == length). The second is a width parameter, defining the size of the wavelet (e.g. standard deviation of a gaussian). See `ricker`, which satisfies these requirements. widths : (M,) sequence Widths to use for transform.
  Returns: | cwt: (M, N) ndarray Will have shape of (len(widths), len(data)).

  Notes

      >>> length = min(10 * width[ii], len(data))
      >>> cwt[ii,:] = scipy.signal.convolve(data, wavelet(length,
      ...                                       width[ii]), mode='same')

  Examples

      >>> from scipy import signal
      >>> import matplotlib.pyplot as plt
      >>> t = np.linspace(-1, 1, 200, endpoint=False)
      >>> sig  = np.cos(2 * np.pi * 7 * t) + signal.gausspulse(t - 0.4, fc=2)
      >>> widths = np.arange(1, 31)
      >>> cwtmatr = signal.cwt(sig, signal.ricker, widths)
      >>> plt.imshow(cwtmatr, extent=[-1, 1, 1, 31], cmap='PRGn', aspect='auto',
      ...            vmax=abs(cwtmatr).max(), vmin=-abs(cwtmatr).max())
      >>> plt.show()

  (Source code)