#### Previous topic

scipy.signal.freqresp

#### Next topic

scipy.signal.lti.A

# scipy.signal.lti

class `scipy.signal.``lti`(*system)

  Linear Time Invariant system base class.

  Parameters: | *system : arguments The `lti` class can be instantiated with either 2, 3 or 4 arguments. The following gives the number of arguments and the corresponding subclass that is created: 2: `TransferFunction`: (numerator, denominator) 3: `ZerosPolesGain`: (zeros, poles, gain) 4: `StateSpace`: (A, B, C, D) Each argument can be an array or a sequence.

  Notes

  `lti` instances do not exist directly. Instead, `lti` creates an instance of one of its subclasses: `StateSpace`, `TransferFunction` or `ZerosPolesGain`.

  Changing the value of properties that are not directly part of the current system representation (such as the `zeros` of a `StateSpace` system) is very inefficient and may lead to numerical inaccuracies.

  Attributes

  `A` | A matrix of the `StateSpace` system.
  `B` | B matrix of the `StateSpace` system.
  `C` | C matrix of the `StateSpace` system.
  `D` | D matrix of the `StateSpace` system.
  `den` | Denominator of the `TransferFunction` system.
  `gain` | Gain of the `ZerosPolesGain` system.
  `num` | Numerator of the `TransferFunction` system.
  `poles` | Poles of the `ZerosPolesGain` system.
  `zeros` | Zeros of the `ZerosPolesGain` system.

  Methods

  `bode`([w, n]) | Calculate Bode magnitude and phase data of a continuous-time system.
  `freqresp`([w, n]) | Calculate the frequency response of a continuous-time system.
  `impulse`([X0, T, N]) | Return the impulse response of a continuous-time system.
  `output`(U, T[, X0]) | Return the response of a continuous-time system to input U.
  `step`([X0, T, N]) | Return the step response of a continuous-time system.