#### Previous topic

scipy.signal.normalize

#### Next topic

scipy.signal.buttord

# scipy.signal.butter

`scipy.signal.``butter`(N, Wn, btype='low', analog=False, output='ba')

  Butterworth digital and analog filter design.

  Design an Nth-order digital or analog Butterworth filter and return the filter coefficients.

  Parameters: | N : int The order of the filter. Wn : array_like A scalar or length-2 sequence giving the critical frequencies. For a Butterworth filter, this is the point at which the gain drops to 1/sqrt(2) that of the passband (the “-3 dB point”). For digital filters, Wn is normalized from 0 to 1, where 1 is the Nyquist frequency, pi radians/sample. (Wn is thus in half-cycles / sample.) For analog filters, Wn is an angular frequency (e.g. rad/s). btype : {‘lowpass’, ‘highpass’, ‘bandpass’, ‘bandstop’}, optional The type of filter. Default is ‘lowpass’. analog : bool, optional When True, return an analog filter, otherwise a digital filter is returned. output : {‘ba’, ‘zpk’, ‘sos’}, optional Type of output: numerator/denominator (‘ba’), pole-zero (‘zpk’), or second-order sections (‘sos’). Default is ‘ba’.
  Returns: | b, a : ndarray, ndarray Numerator (b) and denominator (a) polynomials of the IIR filter. Only returned if `output='ba'`. z, p, k : ndarray, ndarray, float Zeros, poles, and system gain of the IIR filter transfer function. Only returned if `output='zpk'`. sos : ndarray Second-order sections representation of the IIR filter. Only returned if `output=='sos'`.

  See also

  `buttord`, `buttap`

  Notes

  The Butterworth filter has maximally flat frequency response in the passband.

  The `'sos'` output parameter was added in 0.16.0.

  Examples

  Plot the filter’s frequency response, showing the critical points:

      >>> from scipy import signal
      >>> import matplotlib.pyplot as plt

      >>> b, a = signal.butter(4, 100, 'low', analog=True)
      >>> w, h = signal.freqs(b, a)
      >>> plt.semilogx(w, 20 * np.log10(abs(h)))
      >>> plt.title('Butterworth filter frequency response')
      >>> plt.xlabel('Frequency [radians / second]')
      >>> plt.ylabel('Amplitude [dB]')
      >>> plt.margins(0, 0.1)
      >>> plt.grid(which='both', axis='both')
      >>> plt.axvline(100, color='green') # cutoff frequency
      >>> plt.show()

  (Source code)