To be a Client in BEM

For a COMPORT connection:
   1. Get the phone number from the Server person and a sense of how long
      before they will be up and running.
   2. Double-click on the Modem object in the Client folder.
   3. When asked, enter your COMPORT and the PHONE NUMBER that you will be
      using.
   4. Wait for the connection to be established, then...
   5. PLAY BEM!!!

For an Internet/other TCPIP connection:
   1. Start your SLIP connection and get in touch with the Server person
      through email or IRC.
   2. Get the hostname or IP address and your port number from the Server
      person.
   3. Double-click on the Internet/TCPIP object in the Client folder.
   4. When asked, enter the HOSTNAME or IP ADDRESS of the Server and your
      PORT NUMBER.
   4. Wait for the connection to be established, then...
   5. PLAY BEM!!!

For a Direct connection (two machines connected by a serial cable):
   1. Double-click on the Direct-Connect object in the Client folder.
   2. Wait for the connection to be established, then...
   3. PLAY BEM!!!


Troubleshooting:

Note that YAK is running minimized.  If you receive any communication
errors, go to the window list and CLOSE YAK.

