
                  OS/2 PRINT SUBSYSTEM PRINTER DRIVER
                    FIXPAK FOR OS/2 2.11 AND ABOVE

                              IMPORTANT
                              ---------
    PLEASE READ THE FOLLOWING TERMS AND CONDITIONS. DOWNLOADING
    THE SERVICE FIX THAT FOLLOWS, INDICATES YOUR ACCEPTANCE OF THE
    FOLLOWING TERMS AND CONDITIONS:

    - YOU MUST BE, AND YOU AGREE THAT YOU ARE, A PRIOR LICENSEE OF OS/2
      VERSION 2.11 AND ABOVE
    - YOU MAY MAKE COPIES OF THE OS/2 VERSION 2.11 AND ABOVE SERVICE FIX
      EQUAL TO THE NUMBER OF LICENSED COPIES OF OS/2 VERSION 2.11 AND
      AND ABOVE YOU POSSESS
    - YOU MAY ONLY USE THIS SERVICE FIX FOR MAINTENANCE PURPOSES
    - ALL OTHER TERMS AND CONDITIONS OF YOUR OS/2 VERSION 2.11 AND ABOVE
      LICENSE AGREEMENT APPLY TO THIS SERVICE FIX; HOWEVER, THIS DOES NOT
      EXTEND ANY WARRANTY OUTLINED IN SUCH AGREEMENT.

DISKETTE CREATION NOTES
-----------------------
1) To create a diskette from the disk image file you need LOADDSKF.EXE.
   This is also available from the same place you got this FixPak from
   as

   LDF.COM - Self extracting file that will create LOADDSKF.EXE.
             Place in a separate directory on your harddisk then
             enter LDF.

      - or -

   LOADDSKF.ZIP - File compressed with PKZIP, contains LOADDSKF.EXE.
                  Requires PKUNZIP or UNZIP to extract original files
                  from compressed file.

   Use LOADDSKF.EXE to create a diskette. Insert a 2MB HD (1.44MB formatted
   diskette in A:

   a. Enter LOADDSKF XR0Px13.DSK A: /F/Q/Y
       Where x=A, B, C, etc.
       Label OS/2 Printer FixPak XR0Px13


ENHANCED PRINTER DRIVER FIXPAK NAMING CONVENTION
------------------------------------------------
So that customers can more readily identify if a new printer FixPak is
available, an enhancement has been made to the naming convention for printer
FixPaks.  Instead of the normal naming convention of XR0P0nn, XR0PAnn will
be used for the printer FixPak name.   Subsequent printer FixPak releases
will sequentially update the fifth value in the name to allow customers to
differentiate between the different levels of FixPaks.

OS/2 PRINTER FIXPAK NAME = XR0PB13
----------------------------------

PRINTER DRIVER LEVEL = 30.513
-----------------------------

FILES INCLUDED IN THIS FIXPAK ARE:
-----------------------------------
README.1ST - INSTALLATION INSTRUCTIONS (THIS FILE)
README2    - LIST OF APARS FIXED
OMNI.DR_   - OMNI.DRV AND OMNI.HLP MODULES
OMNI.EA_   - OMNI DRIVER EAs
OMNI.SYM   - OMNI DRIVER SYMBOL FILE (FOR DEBUGGING ONLY)

APARS FIXED
-----------
Please see the README2 file for a list of APARs
fixed in this FixPak.

TO INSTALL THIS FIX PERFORM THE FOLLOWING STEPS :
-----------------------------------------------
 Use these printer drivers as you would your original printer
 driver diskettes that were shipped with OS/2.

 - Unpack printer driver with LOADDSKF to a directory on your system
   or to a diskette
 - Open the printer object(s) and deselect all drivers you have
   acquired this fix for and select another driver file as default.
 - Close the printer object.
 - Reboot the system without letting any print jobs print.
 - Open the printer object settings and printer driver and select
   install from one of the driver objects.
 - The "Install New Printer Driver" dialog will appear.
 - Select "Other OS/2 Printer Driver" and enter the drive and/or
   directory that you have put the driver files into for the install.
 - Press Install button and a message box will appear asking if you
   would like to replace the driver with the new level and select yes.
 - Close the "Install New Printer Driver" dialog and select the correct
   driver for the print object
 - Close print object.

You will now be ready to print using the driver.  If you need additional
help installing the printer driver, please refer to the on-line help
facility.

Note 1:
------
If you are in a network environment, we suggest that you match printer
driver levels between both the server and the requestors.

PRINTER DEVICES ADDED SINCE WARP
--------------------------------
Canon BJ-100
Canon BJ-200
Canon BJ-200e
Canon BJ-230
Canon BJ-30
Canon BJC-210
Canon BJC-240
Canon BJC-4000
Canon BJC-4100
Canon BJC-4200
Canon BJC-4550
Canon BJC-5500
Canon BJC-600
Canon BJC-600e
Canon BJC-610
Canon BJC-70
Canon BJC-800
Canon BJC-820
Citizen Notebook Printer II
Citizen PN60
HP DeskJet 340
HP DeskJet 400
HP DeskJet 600
HP DeskJet 600C
HP DeskJet 660C
HP DeskJet 660Cse
HP DeskJet 680C
HP DeskJet 682C
HP DeskJet 850C
HP DeskJet 855C
HP DeskJet 870C
IBM 4208-502
IBM 5572
IBM 5573
IBM 5575
IBM 5575-F02
IBM 5577
IBM 5579
IBM 5587
LQ-300
LQ-300 Color
LX-300
LX-300 Color
Lexmark WinWriter 150c
MJ-3000CU
MJ-5000C
MJ-500C
MJ-700V2C
MJ-800C
MJ-900C
Olivetti JP 170
Olivetti JP 350
Olivetti JP 360
Olivetti JP 450
Olivetti JP 50
Olivetti JP 70
PassThru
Radio Shack JP 1000
Radio Shack JP 1100
Radio Shack JP 500
Seiko Smart Label Plus
Seiko Smart Label Pro
Stylus 1500
Stylus 200
Stylus 400
Stylus 500
Stylus 800+
Stylus 820
Stylus Color II
Stylus Color IIs
Stylus Pro
Stylus Pro XL
Stylus Pro XL+
TIFF Monochrome
Xerox 4003/4004
