NOTE:  Please also see WARPANN.TXT located in 
/ps/products/os2/warp.update.kit.

OS/2 Warp Printer Presentation Driver FixPak

Version.30.460

OS/2 Warp 3.x FixPak containing APAR fixes. Applies to all
versions of Warp released as of this date.

See the RM1 file for installation instructions (also on Fixpak disk 1
as README.1ST).

Note: This Fixpak contains updates to all of the OS/2 Printer
Presentation Drivers.  These updates are necessary if you are
installing the IBM Developer API Extensions (WARPDAX) for OS/2 which
uses the new Dynamic Job Property support in this csd.

**********************************************************************
This package contains the following files:
    XR_WP16.RM1   *  Instructions, module list\disk layout, etc
    XR_WP16.1DK   *  Presentation Printer FixPak disk image 1 of 2
    XR_WP16.2DK   *  Presentation Printer FixPak disk image 2 of 2

You also need the Corrective Service Facility disks which are available
from \ps\products\os2\fixes\v3.0warp\english-us\wkickr and contain:

    CSFBOOT.1DK    * Corrective Service Facility disk 1 of 2
    CSFBOOT.2DK    * Corrective Service Facility disk 2 of 2

You also need LOADDSKF.EXE to create the diskettes from the image files
which is available from \ps\products\os2\tools\ldf.

Download the files with filetype ending in BIN in BINARY to your
PC. Use LOADDSKF to create the diskettes from the images.

    LOADDSKF.CSFBOOT.1DK A:
    LOADDSKF.CSFBOOT.2DK A:
    LOADDSKF.XR_WP16.1DK A:
    LOADDSKF.XR_WP16.2DK A:
