ocmulgee {evd} | R Documentation

## Maximum Annual Flood Discharges of the Ocmulgee River

### Description

The `ocmulgee` data frame has 40 rows and 2 columns. The columns contain maximum annual flood discharges, in units of 1000 cubed feet per second, from the Ocmulgee River in Georgia, USA at Hawkinsville (upstream) and Macon (downstream), for the years 1910 to 1949. The row names give the years of observation.

### Usage

    data(ocmulgee)

### Format

This data frame contains the following columns:

hawk
  A numeric vector containing maximum annual flood discharges at Hawkinsville (upstream).
macon
  A numeric vector containing maximum annual flood discharges at Macon (downstream).

### Source

Gumbel, E. J. and Goldstein, N. (1964) Analysis of empirical bivariate extremal distributions. J. Amer. Statist. Assoc., 59, 794–816.

[Package evd version 2.1-6 Index]