moogladder2
Prev | Orchestra Opcodes and Operators | Next

## moogladder2

moogladder2 — Moog ladder lowpass filter.

## Description

Moogladder2 is an new digital implementation of the Moog ladder filter based on the work of Antti Huovilainen, described in the paper "Non-Linear Digital Implementation of the Moog Ladder Filter" (Proceedings of DaFX04, Univ of Napoli). This implementation uses approximations to the tanh function and so is faster but less accurate than moogladder.

## Syntax

    asig moogladder2 ain, kcf, kres[, istor]

    asig moogladder2 ain, acf, kres[, istor]

    asig moogladder2 ain, kcf, ares[, istor]

    asig moogladder2 ain, acf, ares[, istor]

## Initialization

istor --initial disposition of internal data space. Since filtering incorporates a feedback loop of previous output, the initial status of the storage space used is significant. A zero value will clear the space; a non-zero value will allow previous information to remain. The default value is 0.

## Performance

asig -- input signal.

kcf/acf -- filter cutoff frequency

kres/ares -- resonance, generally < 1, but not limited to it. Higher than 1 resonance values might cause aliasing, analogue synths generally allow resonances to be above 1.

## Examples

Here is an example of the moogladder2 opcode. It uses the file moogladder2.csd.

Example 544. Example of the moogladder2 opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac   ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o moogladder2.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    instr 1

    kfe  expseg 500, p3*0.9, 1800, p3*0.1, 3000
    asig buzz  1, 100, 20, 1
    kres line .1, p3, .99	;increase resonance
    afil moogladder2 asig, kfe, kres
         outs afil, afil

    endin
    </CsInstruments>
    <CsScore>
    f 1 0 4096 10 1

    i 1 0 10
    e
    </CsScore>
    </CsoundSynthesizer>

## Credits

Author: Victor Lazzarini
Author: John ffitch
April 2016

New in version 6.07

Prev | Up | Next
moogladder | Home | moogvcf