QSI INDI Driver
================

This package provides the INDI driver for Quantum Scientific Imaging CCDs & Filter Wheels.

Requirtments
============

+ INDI >= v0.6 (http://indi.sf.net)

	You need to install both indi and indi-devel to build this package.
	
+ cfitsio

	cfitsio-devel is required to compile support for FITS.
	
+ libusb

	libusb is required.
	
+ QSI Api

	QSI api is required
	
Installation
============

	See INSTALL
	
How to Use
==========

	You can use the QSI INDI Driver in any INDI-compatible client such as KStars or Xephem. 
	
	To run the driver from the command line:
	
	$ indiserver indi_qsi_ccd
	
	You can then connect to the driver from any client, the default port is 7624.
	If you're using KStars, the driver will be automatically listed in KStars' Device Manager,
	no further configuration is necessary.
	 