KNRO INDI Driver
==================

This package provides the INDI driver for Radio Astronomy Supplies' SpectraCyber hydrogen line spectrometer. It supports all the functionality provided by the spectrometer including scanning continuum and spectral channels.

TODO: Add stuff about GNUPlot or other solutions here?

Requirtments
============

+ libindi0 >= v0.6 (http://indi.sf.net)

	You need to install both libindi0 and libindi0-devel to build this package.
	

Installation
============

	See INSTALL
	
How to Use
==========

	You can use the SpectraCyber INDI Driver in any INDI-compatible client such as KStars or Xephem. 
	
	To run the driver from the command line:
	
	$ indiserver indi_spectracyber
	
	You can then connect to the driver from any client, the default port is 7624.
	If you're using KStars, the driver will be automatically listed in KStars' Device Manager,
	no further configuration is necessary.
