#### Previous topic

scipy.signal.sosfilt

#### Next topic

scipy.signal.hilbert

# scipy.signal.sosfilt_zi

`scipy.signal.``sosfilt_zi`(sos)

  Compute an initial state zi for the sosfilt function that corresponds to the steady state of the step response.

  A typical use of this function is to set the initial state so that the output of the filter starts at the same value as the first element of the signal to be filtered.

  Parameters: | sos : array_like Array of second-order filter coefficients, must have shape `(n_sections, 6)`. See `sosfilt` for the SOS filter format specification.
  Returns: | zi : ndarray Initial conditions suitable for use with `sosfilt`, shape `(n_sections, 2)`.

  See also

  `sosfilt`, `zpk2sos`

  Notes

  New in version 0.16.0.

  Examples

  Filter a rectangular pulse that begins at time 0, with and without the use of the zi argument of `scipy.signal.sosfilt`.

      >>> from scipy import signal
      >>> import matplotlib.pyplot as plt

      >>> sos = signal.butter(9, 0.125, output='sos')
      >>> zi = signal.sosfilt_zi(sos)
      >>> x = (np.arange(250) < 100).astype(int)
      >>> f1 = signal.sosfilt(sos, x)
      >>> f2, zo = signal.sosfilt(sos, x, zi=zi)

      >>> plt.plot(x, 'k--', label='x')
      >>> plt.plot(f1, 'b', alpha=0.5, linewidth=2, label='filtered')
      >>> plt.plot(f2, 'g', alpha=0.25, linewidth=4, label='filtered with zi')
      >>> plt.legend(loc='best')
      >>> plt.show()

  (Source code)