#### Previous topic

scipy.io.hb_write

#### Next topic

scipy.io.wavfile.write

# scipy.io.wavfile.read

`scipy.io.wavfile.``read`(filename, mmap=False)

  Open a WAV file

  Return the sample rate (in samples/sec) and data from a WAV file.

  Parameters: | filename : string or open file handle Input wav file. mmap : bool, optional Whether to read data as memory-mapped. Only to be used on real files (Default: False). New in version 0.12.0.
  Returns: | rate : int Sample rate of wav file. data : numpy array Data read from wav file. Data-type is determined from the file; see Notes.

  Notes

  This function cannot read wav files with 24-bit data.

  Common data types: [R93]

  WAV format | Min | Max | NumPy dtype
  --- | --- | --- | ---
  32-bit floating-point | -1.0 | +1.0 | float32
  32-bit PCM | -2147483648 | +2147483647 | int32
  16-bit PCM | -32768 | +32767 | int16
  8-bit PCM | 0 | 255 | uint8

  Note that 8-bit PCM is unsigned.

  References

  [R93] | (1, 2) IBM Corporation and Microsoft Corporation, “Multimedia Programming Interface and Data Specifications 1.0”, section “Data Format of the Samples”, August 1991 http://www-mmsp.ece.mcgill.ca/documents/audioformats/wave/Docs/riffmci.pdf