#### Previous topic

scipy.signal.bilinear

#### Next topic

scipy.signal.firls

# scipy.signal.findfreqs

`scipy.signal.``findfreqs`(num, den, N, kind='ba')

  Find array of frequencies for computing the response of an analog filter.

  Parameters: | num, den : array_like, 1-D The polynomial coefficients of the numerator and denominator of the transfer function of the filter or LTI system, where the coefficients are ordered from highest to lowest degree. Or, the roots of the transfer function numerator and denominator (i.e. zeroes and poles). N : int The length of the array to be computed. kind : str {‘ba’, ‘zp’}, optional Specifies whether the numerator and denominator are specified by their polynomial coefficients (‘ba’), or their roots (‘zp’).
  Returns: | w : (N,) ndarray A 1-D array of frequencies, logarithmically spaced.

  Examples

  Find a set of nine frequencies that span the “interesting part” of the frequency response for the filter with the transfer function

  > H(s) = s / (s^2 + 8s + 25)

      >>> from scipy import signal
      >>> signal.findfreqs([1, 0], [1, 8, 25], N=9)
      array([  1.00000000e-02,   3.16227766e-02,   1.00000000e-01,
               3.16227766e-01,   1.00000000e+00,   3.16227766e+00,
               1.00000000e+01,   3.16227766e+01,   1.00000000e+02])