#### Previous topic

scipy.signal.kaiser_beta

#### Next topic

scipy.signal.minimum_phase

# scipy.signal.kaiserord

`scipy.signal.``kaiserord`(ripple, width)

  Design a Kaiser window to limit ripple and width of transition region.

  Parameters: | ripple : float Positive number specifying maximum ripple in passband (dB) and minimum ripple in stopband. width : float Width of transition region (normalized so that 1 corresponds to pi radians / sample).
  Returns: | numtaps : int The length of the kaiser window. beta : float The beta parameter for the kaiser window.

  See also

  `kaiser_beta`, `kaiser_atten`

  Notes

  There are several ways to obtain the Kaiser window:

  - `signal.kaiser(numtaps, beta, sym=True)`
  - `signal.get_window(beta, numtaps)`
  - `signal.get_window(('kaiser', beta), numtaps)`

  The empirical equations discovered by Kaiser are used.

  References

  Oppenheim, Schafer, “Discrete-Time Signal Processing”, p.475-476.